# Approval Report For Tankers

|  |  |
| --- | --- |
| Vehicle registration number: |  |
| Chassis number: |  |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | |  |  |  |  |  | | Construction: | 1: | The load compartment (tank section) mounted in such a way that it cannot be removed from the chassis without leaving obvious traces: | | | | \_\_\_\_\_  (TIR Convention, Annex 2, Article 2, Paragraph 1 (a) - Explanatory notes  2.2.1 (a - d))  \_\_\_\_\_ |  |  |  |  | |  |  |  | Tank section mounted by bolts and the nut welded to the bolt | |  |  |  |  | |  |  |  | Solid rivets - heavy duty | |  |  |  |  | |  |  |  | Welding | |  |  |  |  |  | | Man hole  covers: | 2: | Man hole covers secure: | | | | \_\_\_\_\_ |  |  |  | Bearings and saddles for locking system secure. RIVETED / WELDED | | (TIR Convention, Annex 2, Article 2, Paragraph 1 (a-b), Explanatory note 2.2.1 (a-b) - see also fig. 1-4 and Annex 6, sketch no. 1-1a).  \_\_\_\_\_ |  |  |  |  | |  |  |  | Handle and operational system for tensioning of the cross-bar or locking system secure: RIVETED / WELDED | |  |  |  |  | |  |  |  | Hinges and hinge pin secure: RIVETED / WELDED | |  |  |  |  | |  |  |  | Customs sealing device secured by welding or by solid rivets - "pop-rivets" or "blind rivets" are NOT allowed: | |  |  |  |  |  | | EXPOSED  pipelines: | 3: | Exposed pipelines and flanges secure: | | | | \_\_\_\_\_ |  |  |  |  | | (TIR Convention, Annex 2, Article 2, Paragraph 1 (a-b), Explanatory note 2.2.1 (a-d))  \_\_\_\_\_ |  |  |  | Pipeline secure - all parts (fittings) assembled by welded. | |  |  |  |  | |  |  |  | Bolts for mounting and assembly of pipeline and flanges secure. RIVETED / WELDED | |  |  |  |  | |  |  |  | End covers and stopcocks secure. | |  |  |  |  |  | | Control  compartment: | 4: | Control compartment secure: | | | |  |  |  |  |  | |  |  |  |  | Structure and components of sufficient strength - sides, floor and roof | |  |  |  |  |  | | (TIR Convention, Annex 2, Article 2, Paragraph 1 (a-b), Explanatory note 2.2.1 (a-b) - see also fig. 1-4 and Annex 6, sketch no. 1-1a). |  |  |  | Control compartment mounted to the vehicle in such way that it cannot be removed without leaving obvious traces. | |  |  |  |  | |  |  |  | Hinges and hinge pins for the door (or cover) secure - "pop-rivets" or "blind rivets" are NOT allowed. | |  |  |  |  | |  |  |  | Customs sealing device secured by welding or by a joining device requiring handling from both sides of the constituent parts. | |  |  |  |  |  | | |

|  |  |
| --- | --- |
| Vehicle registration number: |  |
| Chassis number: |  |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | |  |  |  |  |  | | Discharge pipe and stopcocks | 5: | Discharge pipe - end covers and stopcocks secure: | | | |  |  |  |  | |  |  |  | Pipeline secure - all parts (fittings) assembled by welding. | |  |  |  |  |  | |  |  |  |  | Bolts for mounting and assembly of pipeline and flanges secure. RIVETED / WELDED | | (TIR Convention, Annex 2, Article 2, Paragraphs 1 (a-b), Explanatory note  2.2.1(a-d)). |  |  |  |  | |  |  |  | End covers and stopcocks secure. | |  |  |  |  | |  |  |  | ALL closing systems are fitted with a Customs sealing device. The device must be such that it cannot be removed / replaced without leaving obvious traces. | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  | Vehicles comprising a large number of such closures as valves, stopcocks, manhole covers, flanges and the like must be designed so as to keep the number of Customs seals to a minimum. To this end, neighbouring closures must be interconnected by a common device requiring only one Customs seal, or must be provided with a cover meeting the same purpose | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  |  | |  |  |  |  | Openings made for technical purposes, such as systems for measurement of temperature and pressure, shall be allowed only on the condition that they are fitted in such way that there is no access to the load compartment from the outside. For vehicles equipped with such openings inspect the system carefully. | |  |  |  |  |  | |  |  |  |  |  | | |

|  |  |
| --- | --- |
| Vehicle registration number: |  |
| Chassis number: |  |
| |  |  |  |  |  |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | |  |  |  |  |  | | | | | | | | | Sealing: |  | Required number of Customs seals and protection: | | | | | | | | | | | \_\_\_\_\_ |  |  |  |  | | | | | | | | |  |  |  |  |  | | | | | | | | |  |  |  |  | The vehicle requires: seal(s) for Customs secure sealing. | | | | | | | | |  |  |  |  |  | | | | | | | | |  |  |  |  | CLEARLY INDICATE the number of seals required | | | | | | | | | (TIR Convention, Annex  2, Article 2, Paragraph  1 (b) - Explanatory note: 2.2.1 (b) (f)). |  |  |  |  | | | | | | | | |  | IMPORTANT | | | | | | | | | | |  | In cases where more than ONE Customs seal is required for Customs secure sealing of the vehicle, the number of such seals must be indicated in the Certificate of Approval under point 5. | | | | | | | | | | |  | A sketch or photographs must be attached to the Certificate of Approval, showing the exact location of the Customs seals. | | | | | | | | | | | \_\_\_\_\_  (TIR Convention, Article  16 - and Annex 5). |  |  |  |  | | | | | | | | |  |  |  | The Customs seal(s) is adequately protected. | | | | | | | | |  |  |  |  | | | | | | | | |  |  |  | The vehicle is affixed with a TIR plate as described in Article 16 and Annex 5 of the Convention. | | | | | | | | | DECISION: |  |  |  |  |  |  |  |  |  |  |  | |  |  |  | APPROVED |  |  |  |  |  | REJECTED |  | |  |  |  | The vehicle fulfils the technical conditions as laid down in Annex 2 of the TIR Convention |  |  |  |  |  | The vehicle does NOT fulfil the technical conditions as laid down in Annex 2 of the TIR Convention |  | |  |  |  |  |  |  |  |  |  |  |  | |  |  | | | |  |  |  | | | | |  | Annex 2, Article 1: | | | |  |  | The vehicle is not compliant re. the following issues: | | | | |  | (a) | No goods can be removed from or introduced into, the sealed part of the vehicle without leaving obvious traces of tampering or without breaking the Customs seal; | | |  |  |  |  | |  | |  |  |  | | |  |  |  |  | |  | |  | (b) | Customs seals can be simply and effectively affixed | | |  |  |  |  | |  | |  |  |  | | |  |  |  |  | |  | |  | (c) | The vehicle contain no concealed space where goods may be hidden | | |  |  |  |  | |  | |  |  |  | | |  |  |  |  | |  | |  | (d) | All spaces capable of holding goods are readily accessible for Customs inspection | | |  |  |  |  | |  | |  |  |  | | |  |  |  |  | |  | |  |  |  |  | | | | | | | | |  |  |  | Place and date: | | | | | | | | |  |  |  |  | | | | | | | | |  |  |  |  | | | | | | | | |  |  |  | Signed: | | | | | | | | |  |  |  |  | | | | | | | | |  |  |  |  | | | | | | | | |  |  |  | Signed: | | | | | | | | |  |  |  |  | | | | | | | | |  |  |  |  | | | | | | | | | |