|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ST/SG/AC.10/C.3/2016/17−ST/SG/AC.10/C.4/2016/4 | |
|  | **Secretariat** | | Distr.: General  4 April 2016  Original: English |

**Committee of Experts on the Transport of Dangerous Goods  
and on the Globally Harmonized System of Classification  
and Labelling of Chemicals**

|  |  |
| --- | --- |
| **Sub-Committee of Experts on the Transport  of Dangerous Goods** | **Sub-Committee of Experts on the Globally Harmonized System of Classification and Labelling of Chemicals** |
| **Forty-ninth session** | **Thirty-first session** |
| Geneva, 27 June – 6 July 2016  Item 10 (c) of the provisional agenda  **Issues relating to the Globally Harmonized System of Classification and Labelling of Chemicals: Classification criteria for flammable gases** | Geneva, 5 – 8 July 2016  Item 2 of the provisional agenda  **Joint work with the Sub-Committee of Experts on the Transport of Dangerous Goods (TDG Sub-Committee)** |

Proposal for modification of the classification criteria and hazard communication for flammable gases

Transmitted by the experts from Belgium and Japan on behalf of the informal working group[[1]](#footnote-2) on classification criteria for flammable gases

1. During the December 2015 sessions of the Sub-Committee of Experts on the Transport of Dangerous Goods (TDG Sub-Committee) and the Sub-Committee of Experts on the Globally Harmonized System of Classification and Labelling of Chemicals, (GHS Sub-Committee), the joint TDG-GHS informal working group on classification criteria for flammable gases presented the results of its work consisting of new classification criteria to be used for dividing flammable gases. As noted in the report[[2]](#footnote-3), there was full support for the criteria in option 3 in informal documents INF.15 (TDG Sub-Committee, 48th session) - INF.4 (GHS Sub-Committee, 30th session) i.e., allowing for sub-categorization of current category 1 into category 1A and 1B, with category 1B addressing gases with a lower flammability limit greater than 6% or a fundamental burning velocity of less than 10 cm/s. It was noted that the new sub-category 1B would allow the classification of gases and gas mixtures with a lower burning velocity developed by the refrigeration and foam plastics industries following the phasing down of high global warming potential substances. It was also noted that the criteria in option 3 would not entail any change in classification for transport purposes.

2. As regards the proposed hazard communication elements in informal documents INF.24 (TDG Sub-Committee, 48th session) - INF.7 (GHS Sub-Committee, 30th session) Belgium and Japan agreed to bring forward further information. In addition to this formal proposal the experts from Belgium and Japan submit additional information in an informal document regarding the appropriateness of the signal word and hazard statement (warning/flammable gas) for the proposed category 1B.

3. This document contains the following annexes:

* Annex 1: Proposed amendments to Chapter 2.2 of the GHS
* Annex 2: Consequential amendments to Annex 1, Table A1.2, of the GHS
* Annex 3: Consequential amendments to Annex 3 (Sections 1, 2 and 3) of the GHS
* Annex 4: Consequential amendments to Annex 4, Section 9, of the GHS

4. The TDG and GHS sub-committees are invited to consider the proposal as contained in annexes 1 to 4 to this document. Changes to the current text in the GHS are shown using the “track-changes” function.

Annex 1

Proposed amendments to Chapter 2.2 of the GHS

“CHAPTER 2.2  
FLAMMABLE GASES

2.2.1 Definitions

2.2.1.1 A *flammable gas* is a gas having a flammable range with air at 20 °C and a standard pressure of 101.3 kPa.

2.2.1.2 A *pyrophoric gas* is a flammable gas that is liable to ignite spontaneously in air at a temperature of 54 ºC or below.

2.2.1.3 A *chemically unstable gas* is a flammable gas that is able to react explosively even in the absence of air or oxygen.

2.2.2 Classification criteria

2.2.2.1

A flammable gas is classified in Category 1 or 2 according to the following table. Pyrophoric and/or chemically unstable gases are always classified in Category 1. Gases classified in Category 1, but which are not pyrophoric and/or chemically unstable, may be further categorized on the basis of the lower flammability limit (LFL) or the fundamental burning velocity (FBV) (see Table 2.2.1).

**Table 2.2.1: Criteria for categorisation of flammable gases**

|  |  |
| --- | --- |
| **Category** | **Criteria** |
| **1/1A** | Gases, which at 20 °C and a standard pressure of 101.3 kPa:  (a) are ignitable when in a mixture of 13% or less by volume in air; or  (b) have a flammable range with air of at least 12 percentage points regardless of the lower flammability limit. |
| **1B** | Gases which meet the criteria of category 1/1A and which have at least either:   1. A lower flammability limit of more than 6% by volume in air; or   b) A fundamental burning velocity of less than 10 cm/s; |
| **2** | Gases, other than those of Category 1, which, at 20 °C and a standard pressure of 101.3 kPa, have a flammable range while mixed in air. |

***NOTE 1****: Ammonia and methyl bromide may be regarded as special cases for some regulatory purposes.*

***NOTE 2:*** *Aerosols should not be classified as flammable gases. See Chapter 2.3.*

2.2.2.2 A flammable gas is additionally classified as pyrophoric if it meets the criteria in the following table:

**Table 2.2.2: Criteria for pyrophoric gases**

|  |  |
| --- | --- |
| Category | Criteria |
| Pyrophoric gas | Flammable gas that ignite spontaneously in air at a temperature of 54 ºC or below. |

***NOTE 1:*** *Spontaneous ignition for pyrophoric gases is not always immediate, and there may be a delay.*

***NOTE 2:*** *In the absence of data on its pyrophoricity, a flammable gas mixture should be classified as a pyrophoric gas if it contains more than 1% (by volume) of pyrophoric component(s).*

2.2.2.3 A flammable gas that is also chemically unstable is additionally classified in one of the two categories for chemically unstable gases using the methods described in Part III of the Manual of Tests and Criteria according to the following table:

**Table 2.2.3: Criteria for chemically unstable gases**

|  |  |
| --- | --- |
| Category | Criteria |
| A | Flammable gases which are chemically unstable at 20°C and a standard pressure of 101.3 kPa |
| B | Flammable gases which are chemically unstable at a temperature greater than 20°C and/or a pressure greater than 101.3 kPa |

2.2.3 Hazard communication

2.2.3.1 General and specific considerations concerning labelling requirements are provided in *Hazard communication: Labelling* (Chapter 1.4). Annex 1 contains summary tables about classification and labelling. Annex 3 contains examples of precautionary statements and pictograms which can be used where allowed by the competent authority.

## **Table 2.2.4: Label elements for flammable gases**

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Flammable gas** | | | **Additional categories** | | |
| **Pyrophoric gas** | **Chemically unstable gas** | |
| **Category 1/1A** | **Category 1B** | **Category 2** | **Pyrophoric gas** | **Category A** | **Category B** |
| **Symbol** | Flame | [Flame] | *No symbol* | Flame | Flame | Flame |
| **Signal word** | Danger | [Danger]/ [Warning] | Warning | Danger | Danger | Danger |
| **Hazard statement** | Extremely flammable gas | [Flammable gas]/ [Highly flammable gas] | Flammable gas | Extremely flammable gas  May ignite spontaneously if exposed to air | Extremely flammable gas  May react explosively even in the absence of air | Extremely flammable gas  May react explosively even in the absence of air at elevated pressure and/or temperature |

2.2.3.2 If a flammable gas or gas mixture is additionally classified in one or more sub-categories, then all relevant classification(s) should be communicated on the safety data sheet as specified in Annex 4, and the relevant hazard communication elements included on the label.

2.2.4 Decision logic and guidance

The decision logic and guidance, which follow, are not part of the harmonized classification system, but have been provided here as additional guidance. It is strongly recommended that the person responsible for classification studies the criteria before and during use of the decision logic.

2.2.4.1 *Decision logic for flammable gases*

To classify a flammable gas, data on its flammability, on its ability to ignite in air and on its chemical instability are required. In case of further categorisation within category 1, data on its lower flammability limit or its fundamental burning velocity is required. The classification is according to decision logic 2.2 .

*Decision logic 2.2* FOOTNOTE [[3]](#footnote-4)1

**2.2.4.2 *Guidance***

Yes

Optional

Category 1A



Danger

Category 1B



[Danger]/[Warning]

Is the LFL > 6% by volume in air ; or

Is the FBV < 10 cm/s ?

No

2.2.4.2.1 Flammability should be determined by tests or by calculation in accordance with methods adopted by ISO (see ISO 10156:2010 “Gases and gas mixtures – Determination of fire potential and oxidizing ability for the selection of cylinder valve outlets” and, if using fundamental burning velocity for Category 1B, see ISO 817:2014 “Refrigerants-Designation and safety classification, Annex C : Method of test for burning velocity measurement of flammable gases”). Where insufficient data are available to use these methods, tests by a comparable method recognized by the competent authority may be used.

2.2.4.2.2 Pyrophoricity should be determined at 54°C in accordance with either IEC 60079-20-1 ed1.0 (2010-01) “Explosive atmospheres – Part 20-1: Material characteristics for gas and vapour classification – Test methods and data” or DIN 51794 “Determining the ignition temperature of petroleum products”.

2.2.4.2.3 The classification procedure for pyrophoric gases need not be applied when experience in production or handling shows that the substance does not ignite spontaneously on coming into contact with air at a temperature of 54 ºC or below. Flammable gas mixtures, which have not been tested for pyrophoricity and contain more than one percent pyrophoric components, should be classified as a pyrophoric gas. Expert judgement on the properties and physical hazards of pyrophoric gases and their mixtures should be used in assessing the need for classification of flammable gas mixtures containing one percent or less pyrophoric components. In this case, testing need only be considered if expert judgement indicates a need for additional data to support the classification process.

2.2.4.2.4 Chemical instability should be determined in accordance with the method described in Part III of the Manual of Tests and Criteria. If the calculations in accordance with ISO 10156:2010 show that a gas mixture is not flammable it is not necessary to carry out the tests for determining chemical instability for classification purposes.

2.2.5 Example: Classification of a flammable gas mixture by calculation according to ISO 10156:2010

Formula



where:

Vi % = the equivalent flammable gas content;

Tci = the maximum concentration of a flammable gas in nitrogen at which the mixture is still not flammable in air;

i = the first gas in the mixture;

n = the nth gas in the mixture;

Ki = the equivalency factor for an inert gas versus nitrogen;

Where a gas mixture contains an inert diluent other than nitrogen, the volume of this diluent is adjusted to the equivalent volume of nitrogen using the equivalency factor for the inert gas (Ki).

Criterion

**

Gas mixture

For the purpose of this example the following is the gas mixture to be used

2% (H2) + 6%(CH4) + 27%(Ar) + 65%(He)

Calculation

1. Ascertain the equivalency factors (Ki) for the inert gases versus nitrogen:

Ki (Ar) = 0.5

Ki (He) = 0.5

2. Calculate the equivalent mixture with nitrogen as balance gas using the Ki figures for the inert gases:

2%(H2) + 6%(CH4) + [27% × 0.5 + 65% × 0.5](N2) = 2%(H2).+ 6%(CH4) + 46%(N2) = 54%

3. Adjust the sum of the contents to 100%:

 × [2%(H2) + 6%(CH4) + 46%(N2)] = 3.7%(H2) + 11.1%(CH4) + 85.2%(N2)

4. Ascertain the Tci coefficients for the flammable gases:

Tci H2 = 5.7%

Tci CH4 = 14.3%

5. Calculate the flammability of the equivalent mixture using the formula:

 =  +  = 1.42 **1.42 > 1**

Therefore the mixture is flammable in air.”

Annex 2

Consequential amendments to Annex 1, Table A1.2 of the GHS

**“A1.2 Flammable gases** (see Chapter 2.2 for classification criteria)

| **Classification** | | **Labelling** | | | | **Hazard statement codes** |
| --- | --- | --- | --- | --- | --- | --- |
| **Hazard class** | **Hazard category** | **Pictogram** | | **Signal word** | **Hazard statement** |
| **GHS** | **UN Model Regulationsa** |
| **Flammable gases** | **1/1A** | **Description: Beskrivning: H:\Mina Dokument\KemI Internationellt\GHS\Pictograms\flamme.tif** | **Description: Beskrivning: H:\Mina Dokument\KemI Internationellt\GHS\Pictograms\rouge2.tif** | **Danger** | Extremely flammable gas | H220 |
| **1B** | **Description: Beskrivning: H:\Mina Dokument\KemI Internationellt\GHS\Pictograms\flamme.tif** | **Description: Beskrivning: H:\Mina Dokument\KemI Internationellt\GHS\Pictograms\rouge2.tif** | **[Danger]/ [Warning]** | **[Flammable gas]/[Highly flammable gas]** | H221 |
| **2** | *No pictogram* | *Not required* | **Warning** | Flammable gas | H221 |
| **Pyrophoric gas** |  |  | **Danger** | Extremely flammable gas | H220 |
| May ignite spontaneously if exposed to air | H232 |
| **A**  **(chemically unstable gases)** |  | *(Not applicable)b* | *Danger* | Extremely flammable gas | H220 |
| May react explosively even in the absence of air | H230 |
| **B**  **(chemically unstable gases)** |  | *(Not applicable)b* | *Danger* | Extremely flammable gas | H220 |
| May react explosively even in the absence of air at elevated pressure and/or temperature | H231 |

a *Under the UN Recommendations on the Transport of Dangerous Goods, Model Regulations, the symbol, number and border line may be shown in black instead of white. The background colour stays red in both cases.”*

b *Chemically unstable gases are not authorized for transport.*

Annex 3

Consequential amendments to Annex 3 of the GHS

Section 1, Table A3.1.1

**For H220**

In column 4, under “hazard category”, replace “1” with “1/1A”.

**For H221**

In column 4, under “hazard category”, replace “2” with “1B, 2”.

Section 2, Table A3.2.2

**For P210**

In column (4), under “hazard category”, for “flammable gases” replace “1, 2” with “1/1A, 1B, 2”

Section 2, Table A3.2.3

**For P377**

In column (4), under “hazard category”, for “flammable gases” replace “1, 2” with “1/1A, 1B, 2”

**For P381**

In column (4), under “hazard category”, for “flammable gases” replace “1, 2” with “1/1A, 1B, 2”

Section 2, Table A3.2.4

**For P403**

In column (4), under “hazard category”, for “flammable gases” replace “1, 2” with “1/1A, 1B, 2”

Section 3, paragraph A3.3.5

Amend the matrix tables for flammable gases as follows:

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **FLAMMABLE GASES**  **(Chapter 2.2)**  **(Flammable gases)** | | | | | | | |
|  |  | |  | | | | **Symbol**  Flame |
| **Hazard category** | **Signal word** | | **Hazard statement** | | | |  |
| 1/1A | Danger | | H220 | Extremely flammable gas | | |
| **Precautionary statements** | | | | | | | |
| **Prevention** | | **Response** | | | **Storage** | **Disposal** | |
| P210 **Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking.** | | P377 **Leaking gas fire: Do not extinguish, unless leak can be stopped safely.**  P381 **In case of leakage, eliminate all ignition sources.** | | | P403 **Store in a well-ventilated place.** |  | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **FLAMMABLE GASES**  **(Chapter 2.2)**  **(Flammable gases)** | | | | | | | |
|  |  | |  | | | | **Symbol**  Flame |
| **Hazard category** | **Signal word** | | **Hazard statement** | | | |  |
| 1B | [Danger]/[Warning] | | H221 | [Flammable gas]/[Highly Flammable Gas] | | |
| **Precautionary statements** | | | | | | | |
| **Prevention** | | **Response** | | | **Storage** | **Disposal** | |
| P210 **Keep away from heat, hot surfaces, sparks, open flames and other ignition sources. No smoking.** | | P377 **Leaking gas fire: Do not extinguish, unless leak can be stopped safely.**  P381 **In case of leakage, eliminate all ignition sources.** | | | P403 **Store in a well-ventilated place.** |  | |

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **FLAMMABLE GASES**  **(CHAPTER 2.2)**  **(Pyrophoric gases)** | | | | | | | |
|  |  | |  | | | | **Symbol**  Flame |
| **Hazard category** | **Signal word** | | **Hazard statement** | | | |  |
| Pyrophoric gas | Danger | | H220  H232 | Extremely flammable gas  May ignite spontaneously if exposed to air | | |
| **Precautionary statements** | | | | | | | |
| **Prevention** | | **Response** | | | **Storage** | **Disposal** | |
| P222 **Do not allow contact with air. –** *if emphasis of the hazard statement is deemed necessary.*  P280 **Wear protective gloves/protective clothing/eye protection/face protection.** Manufacturer/supplier or the competent authority to specify the appropriate type of equipment. | |  | | |  |  | |

***Note****: This table lists only precautionary statements that are assigned due to the pyrophoricity of the gas. For the other precautionary statements that are assigned based on the flammability, see the respective tables for flammable gases.*

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
| **FLAMMABLE GASES**  **(Chapter 2.2)**  **(Chemically unstable gases)** | | | | | | | |
|  |  | |  | | | | **Symbol**  Flame |
| **Hazard category** | **Signal word** | | **Hazard statement** | | | |  |
| A | *Danger* | | H220  H230 | Extremely flammable gas  May react explosively even in the absence of air | | |
| B | *Danger* | | H220  H231 | Extremely flammable gas  May react explosively even in the absence of air at elevated pressure and/or temperature | | |
| **Precautionary statements** | | | | | | | |
| **Prevention** | | **Response** | | | **Storage** | **Disposal** | |
| P202 **Do not handle until all safety precautions have been read and understood.** | |  | | |  |  | |

***Note:*** *This table lists only the precautionary statement that is assigned due to the chemical instability of the gas. For the other precautionary statements that are assigned based on the flammability see the respective tables for flammable gases.*

Annex 4

Guidance on the preparation of Safety Data Sheets (SDS)

In paragraph A4.3.9, table .A4.3.9.2, amend the text in column 3 for the row applicable to chapter 2.2 as follows :

| **Chapter** | **Hazard class** | **Property/Safety characteristic/Test result and  Remarks/Guidance** |
| --- | --- | --- |
| 2.2 | Flammable gases | for pure flammable gases:  − no data on the explosion / flammability limits is needed because these are indicated based on Table A4.3.9.1  − indicate the *TCi* (maximum content of flammable gas which, when mixed with nitrogen, is not flammable in air, in %) as per ISO 10156  - if the gas is classified as Category 1B on the basis of the Fundamental Burning Velocity (FBV), indicate the FBV, as measured by ISO 817:2014 “Refrigerants-Designation and safety classification, Annex C : Method of test for burning velocity measurement of flammable gases” or another scientific validated method.  for flammable gas mixtures:  − indicate the explosion / flammability limits, if tested (if classification as flammable is based on the calculation as per ISO 10156, assignment of cat. 1 is compulsory)  - if the gas mixture is classified as Category 1B on the basis of the Fundamental Burning Velocity (FBV), indicate the FBV, as measured by ISO 817:2014 “Refrigerants-Designation and safety classification, Annex C : Method of test for burning velocity measurement of flammable gases” or another scientific validated method. |

1. In accordance with the programme of work of the Sub-Committee for 2015–2016 approved by the Committee at its seventh session (see ST/SG/AC.10/C.3/92, paragraph 95 and ST/SG/AC.10/42, para. 15). [↑](#footnote-ref-2)
2. Refer to the report of the GHS Sub-Committee on its 30th session (ST/SG/AC.10/C.4/60, paras. 4 to 8). [↑](#footnote-ref-3)
3. 1 *In the absence of data on its pyrophoricity, a flammable gas mixture should be classified as pyrophorioc gas if it contains more than 1% (by volume) of pyrophoric component(s).* [↑](#footnote-ref-4)