|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2017/74 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  10 April 2017  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**172nd session**

Geneva, 20-23 June 2017

Item 4.10.3 of the provisional agenda

**1958 Agreement: Consideration of draft amendments**

**to existing Regulations submitted by GRE**

Proposal for Supplement 29 to the 01 series of amendments to Regulation No. 6 (Direction indicators)

**Submitted by the Working Party on Lighting and Light-Signalling**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Lighting and Light-Signalling (GRE) at its seventy-seventh session (ECE/TRANS/WP.29/GRE/77). It is based on ECE/TRANS/WP.29/GRE/2017/7 and Annex IV to ECE/TRANS/WP.29/GRE/77. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their June 2017 sessions.

Supplement 29 to the 01 series of amendments to Regulation No. 6 (Direction indicators)

*Paragraph 5.5.1.,* amend to read:

"5.5.1. The device shall only be equipped with light source(s) approved according to Regulation No. 37 and/or Regulation No. 128, provided that no restriction on the use is made in Regulation No. 37 and its series of amendments in force at the time of application for type approval or in Regulation No. 128 and its series of amendments in force at the time of application for type approval."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)