|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2017/106 |
| Description: _unlogo | **Economic and Social Council** | Distr.: General11 April 2017Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**172nd session**

Geneva, 20-23 June 2017

Item 4.10.16 of the provisional agenda

**1958 Agreement: Consideration of draft amendments**

**to existing Regulations submitted by GRE**

Proposal for Supplement 11 to the 05 series of amendments to Regulation No. 48 (Installation of lighting and light-signalling devices)

**Submitted by the Working Party on Lighting and Light-Signalling**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Lighting and Light-Signalling (GRE) at its seventy-seventh session (ECE/TRANS/WP.29/GRE/77). It is based on Annex III to ECE/TRANS/WP.29/GRE/77. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their June 2017 sessions.

Supplement 11 to the 05 series of amendments to Regulation No. 48 (Installation of lighting and light-signalling devices)

*Paragraph 6.5.7.*, amend to read:

"6.5.7. Electrical connections

Direction-indicator lamps shall switch on independently of the other lamps. All direction-indicator lamps on one side of a vehicle shall be switched on and off by means of one control and shall flash in phase.

On M1 and N1 vehicles less than 6 m in length, with an arrangement complying with Paragraph 6.5.5.2. above, the amber side-marker lamps, when mounted, shall also flash at the same frequency (in phase) with the direction indicator lamps.

A direction indicator capable of being activated in different modes (static or sequential), shall not switch between both modes once activated.

If two optional lamps (category 2a or 2b) are installed on vehicles in categories M2, M3, N2, N3, they shall be operated in the same mode as the other mandatory rear direction indicator lamps (category 2a or 2b); i.e. static or sequential."

*Paragraph 6.6.1.*, amend to read:

"6.6.1. Presence

Mandatory.

The signal shall be given by simultaneous operation of the direction-indicator lamps in accordance with the requirements of paragraph 6.5. above.

All direction indicators of the category 1 (1, 1a, 1b) activated simultaneously shall operate in the same mode; i.e. static or sequential.

All direction indicators of the category 2 (2a, 2b) activated simultaneously shall operate in the same mode; i.e. static or sequential."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)