|  |  |
| --- | --- |
| Submitted by the experts from ETRTO | Informal document **GRRF-84-34**  84th GRRF, 19-22 September 2017  Agenda item 7(c) |

**Additional amendment to the Proposal for amendments to Regulation No. 54 (ECE/TRANS/WP.29/GRRF/2017/18)**

The text proposed in ECE/TRANS/WP.29/GRRF/2017/18 does not refer correctly to the proper paragraphs after the renumbering introduced due to the introduction of new paragraphs (ref. Supplement 21). By separating para. 3.1. into paras. 3.1.1. and 3.1.2., paragraph 3.1.12. has become 3.1.13.

*Paragraph 3.4.,* amend to read:

"3.4. The markings referred to in paragraph 3.1. and the approval mark prescribed in paragraph 5.4. of this Regulation shall be moulded on to or into the tyres. They shall be clearly legible and shall, except for the marking referred to in paragraph**s** 3.1.1.**, 3.1.2. and 3.1.~~12.~~13.** above, be located on at least one lower sidewall."