|  |  |  |
| --- | --- | --- |
|  |  | **INF.10** |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**104th session 13 April 2018**

Geneva, 15-17 May 2018

Item 5 (a) of the provisional agenda

**Proposals for amendments to annexes A and B of ADR**

**construction and approval of vehicles**

 The interpretation of Section 9.2.5 «Speed limitation device» ADR

 Transmitted by the Government of the Russian Federation

 Introduction

At the 101st session of the Working Party on the Transport of Dangerous Goods the Russian Federation presented the document ECE/TRANS/WP.15/2016/13 with a proposal
to consider the possibility of applying not only a separate speed limitation device (SLD)
as an implementation of ADR section 9.2.5, but also speed limitation function (SLF).

The Working Party invited the representatives of the Russian Federation to also consult
the Working Party on Braking and Running Gear of the World Forum for Harmonization
of Vehicle Regulations (WP.29) and, as a result, prepare a proposal for amending Section 9.2.5 at a future session.

The eighty-sixth session of the Working Party on Braking and Running Gear (GRRF) was held from 12 to 16 February, 2018, at which the Russian Federation initiated
the consideration of this issue.

In accordance with paragraph 57 of the report of the eighty-sixth session of the Working Party on Braking and Running Gear (ECE/TRANS/WP.29/GRRF/86) GRRF confirmed that a vehicle equipped with a speed limitation function (SLF) would comply with ADR section 9.2.5, similar to a vehicle equipped with a speed limitation device (SLD).

 Proposal

1. Adopt the conclusions of the GRRF session.

2. Add the following changes to ADR section 9.2.5 (the proposals for changes are underlined or crossed out)

«Motor vehicles (rigid vehicles and tractors for semi-trailers) with a maximum mass exceeding 3.5 tonnes, shall be equipped with a speed limitation device or a speed limitation function according to the technical requirements of ECE Regulation
No. 895, as amended. The speed limitation device or function shall be set in such a way that the speed cannot exceed 90 km/h, bearing in mind the technological tolerance
of the device.»

3. Consider the possibility of applying these changes from 2019 onwards.