|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2019/125 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  27 August 2019  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**179th session**

Geneva, 12-14 November 2019

Item 4.6.5 of the provisional agenda

**1958 Agreement:  
consideration of draft amendments to existing   
UN Regulations submitted by GRE**

Proposal for Supplement 2 to the original series of UN Regulation No. [149] (Road Illumination Devices)

Submitted by the Informal Working Group on Simplification of Lighting and Light-Signalling Regulations[[1]](#footnote-2)\*

The text reproduced below was prepared by the Informal Working Group on Simplification of Lighting and Light-Signalling Regulations (IWG SLR) with the aim to correct errors inadvertently introduced in the text of the new UN Regulation No. [149] (ECE/TRANS/WP.29/2018/158/Rev.1) which is expected to come into force on 15 November 2019. The proposal will be adopted by the Working Party on Lighting and Light-Signalling (GRE) at its session in October 2019 (ECE/TRANS/WP.29/GRE/82). It is based on informal document GRE-82-02.

Supplement 2 to the original series of UN Regulation No. [149] (Road Illumination Devices)

*Paragraph 5.2.2., table 8, part A, No. 7,* amend to read:

“5.2.2. …

# Table 8

# Luminous intensities of passing-beam (all intensities expressed in cd)

|  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | … | | | | | | | | | | |
|  | 7 | 50L | 3.43 L |  | 0.86 D |  | 13,200\* |  | 13,200\* |  | 18,480 |
|  | … | | | | | | | | | | |

…”

*Paragraph 5.3.2.8.2., table 13,* amend to read:

“5.3.2.8.2. …

# Table 13

# Overhead sign requirements, angular position of measurement points

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Point designation | S50LL | S50 | S50RR | S100LL | S100 | S100RR |
| Angular position in degrees | 4 U / 8 L | 4 U / V-V | 4 U / 8 R | 2 U / 4 L | 2 U / V-V | 2 U / 4 R |

# …”

1. \* In accordance with the programme of work of the Inland Transport Committee for 2018–2019 (ECE/TRANS/274, para. 123 and ECE/TRANS/2018/21/Add.1, cluster 3.1), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)