Proposed amendments to ECE/TRANS/WP.29/GRSG/2019/2

Revised proposal for Supplement 4 to the 03 series of amendments to UN R 26

**I. Proposal**

*Paragraph 6.8.1.,* amend to read:

"6.8.1. Sheet-metal edges, such as gutter edges and the rails of sliding doors, shall not be permitted unless they are folded back or are fitted with a shield meeting the requirements of this Regulation which are applicable to it.

 An unprotected edge shall be considered to be folded back either if it is folded back by approximately 180º, or if it is folded towards the bodywork in such a manner that it cannot be contacted by a sphere having a diameter of 100 mm.

 The requirements of paragraph 5.4. above shall not apply to the following sheet metal edges: rear edge of bonnet and front edge of rear luggage boot.

 **The rear edge of the bonnet includes the extrapolation of this edge to the left and right (e.g. as upper edge of the fender or as edge of the a-pillar). This extrapolation is limited laterally by the outermost lateral point of the windscreen glass ~~and other inward facing edges of body panels not easily contacted by vulnerable road users may be blunted.~~**~~"~~

 II. Justification

 See original document