|  |  |
| --- | --- |
|  | E/ECE/324/Rev.1/Add.15/Rev.8/Amend.1−E/ECE/TRANS/505/Rev.1/Add.15/Rev.8/Amend.1 |
|  |  | 11 July 2016 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 15 – Regulation No. 16

 Revision 8 - Amendment 1

Supplement 6 to the 06 series of amendments – Date of entry into force: 18 June 2016

 Uniform provisions concerning the approval of:

I. Safety-belts, restraint systems, child restraint systems and ISOFIX child restraint systems for occupants of power-driven vehicles

II. Vehicles equipped with safety-belts, safety-belt reminder, restraint systems, child restraint systems, ISOFIX child restraint systems and i-Size child restraint systems

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2015/93

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Paragraph 6.2.2.2*., amend to read:

"6.2.2.2. The buckle, even when … … The buckle release area shall be coloured red. No other part of the buckle shall be of this color. When the seat is occupied, a red warning light as part of the buckle shall be permitted, if it is switched off by the action of buckling the seat belt. Lights illuminating the buckle in a colour other than red are not required to be switched off by the action of buckling the seat belt. These lights shall not illuminate the buckle in such a way that the perception of the red colour of the buckle release or the red of the warning light is affected."

*Paragraph 7.7.1.*, amend to read:

"7.7.1. The belt assembly shall be mounted on a trolley equipped with the seat and the general anchorages as defined in Annex 6, Figure 1, to this Regulation. However, if the belt assembly is intended ... … the maximum number of real anchorage points."

*Annex 1B,*

*Item 12.*, amend to read:

"12. Approval granted/refused/extended/withdrawn2 for fixation to the general anchorage positions as defined in Annex 6, Figure 1, to this Regulation/for use in a specific vehicle or in specific types of vehicles.2, 4 "

*Annex 6,*

*Paragraph 3.2.*, amend to read:

"3.2. The general anchorages shall be … …"

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)