|  |
| --- |
| **UN/SCETDG/47/INF.55** |
| **Committee of Experts on the Transport of Dangerous Goodsand on the Globally Harmonized System of Classificationand Labelling of Chemicals****Sub-Committee of Experts on the Transport of Dangerous Goods 25 June 2015****Forty-seventh session**Geneva, 22 – 26 June 2015Item 6 (f) of the provisional agenda**Miscellaneous proposals for amendments to the Model Regulations on the Transport of Dangerous Goods: other miscellaneous proposals** |

 Review of the wording of certain amendments to the 18th revised edition of the Model Regulations

 Transmitted by the International Air Transport Association (IATA)

 Proposal

1. Revise 2.2.4 as follows:

“**2.2.4** **Gases not authorized for transport**

Chemically unstable gases of Class 2 are forbidden for transport unless the necessary precautions have been taken to prevent the possibility of a dangerous decomposition or polymerization under normal conditions of transport or unless transported in accordance with special packing provision (r) of packing instruction P200 (4) of 4.1.4.1, as applicable. For the precautions necessary to prevent polymerization, see special provision 386 of Chapter 3.3. To this end particular care shall be taken to ensure that receptacles and tanks do not contain any substances liable to promote these reactions.”.

2. Revise 2.3.5 as follows:

**“2.3.5 Substances not authorized for transport**

Chemically unstable substances of Class 3 are forbidden for transport unless the necessary precautions have been taken to prevent the possibility of a dangerous decomposition or polymerization under normal conditions of transport. For the precautions necessary to prevent polymerization, see special provision 386 of Chapter 3.3. To this end particular care shall be taken to ensure that receptacles and tanks do not contain any substances liable to promote these reactions.”.

3. Revise 2.6.2.5 as follows:

“**2.6.2.5 *Substances not authorized for transport***

Chemically unstable substances of Division 6.1 are forbidden for transport unless the necessary precautions have been taken to prevent the possibility of a dangerous decomposition or polymerization under normal conditions of transport. For the precautions necessary to prevent polymerization, see special provision 386 of Chapter 3.3. To this end particular care shall be taken to ensure that receptacles and tanks do not contain any substances liable to promote these reactions.”.

4. Revise 2.8.3 as follows:

“**2.8.3 Substances not authorized for transport**

Chemically unstable substances of Class 8 are forbidden for transport unless the necessary precautions have been taken to prevent the possibility of a dangerous decomposition or polymerization under normal conditions of transport. For the precautions necessary to prevent polymerization, see special provision 386 of Chapter 3.3. To this end particular care shall be taken to ensure that receptacles and tanks do not contain any substances liable to promote these reactions.”.

5. Special Provision 204 revise the last paragraph as follows:

“Articles containing smoke-producing substance(s) toxic by inhalation according to the criteria for Division 6.1 shall be labelled with a “TOXIC” subsidiary risk label (Model No 6.1, see 5.2.2.2.2), except that those manufactured before 31 December 2016 may be consigned for transport until 31 December 2018 without a “TOXIC” subsidiary label.”.