|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ST/SG/AC.10/C.3/2016/59 | |
| _unlogo | **Secretariat** | | Distr.: General  2 September 2016  Original: English |

**Committee of Experts on the Transport of Dangerous Goods  
and on the Globally Harmonized System of Classification  
and Labelling of Chemicals**

Sub-Committee of Experts on the Transport of Dangerous Goods

**Fiftieth session**

Geneva, 28 November-6 December 2016  
Item 2 (c) of the provisional agenda  
**Recommendations made by the Sub-Committee   
on its forty-seventh, forty-eighth and   
forty-ninth sessions and pending issues:   
listing, classification and packing**

Proposal to modify P902

Transmitted by the Council on Safe Transportation of Hazardous Articles (COSTHA)[[1]](#footnote-2)

Introduction

1. During the forty-ninth session of the Sub-Committee, COSTHA presented revised text for P902 and an example competent approval to clarify that unpackaged articles may be contained in dedicated handling devices when transported to, from, or between a safety device manufacturer and an assembly plant including intermediate handling locations informal documents INF.57 and INF.57/Add.1 (49th session).

2. The Sub-Committee provided general support for the text as written, and therefore COSTHA is proposing to revise the sentence relative to unpackaged articles as presented at the forty-ninth session.

Proposal

3. COSTHA proposes to modify the sentence under the heading **Unpackaged articles** in P902:

The articles may also be transported unpackaged in dedicated handling devices, vehicles or containers when moved to, from, or between where they are manufactured ~~to~~ and an assembly plant including intermediate handling locations.

1. In accordance with the programme of work of the Sub-Committee for 2015–2016 approved by the Committee at its seventh session (see ST/SG/AC.10/C.3/92, paragraph 95 and ST/SG/AC.10/42, para. 15). [↑](#footnote-ref-2)