**Proposal for amendments to Regulation No. 110 (CNG and LNG vehicles)**

**Editorial correction of formal document ECE/TRANS/WP.29/GRSG/2016/8:**

I. Proposal

*Annex 4B, paragraph 1.6.2.2.,* amend to read:

~~"1.6.2.2. The sealing cone of swivel-nut type shall be of the type with a half vertical angle of 45°.~~**~~The interface type for the hose coupling shall be chosen as to comply with the tests described in paragraph 1.7., as well as the tests mentioned in Annexes 5A and 5B~~**~~.~~

 **~~In case of an interface type using a soft seal body (e.g. O-ring), the type of material chosen shall be tested in accordance with Annexes 5D, 5F and 5G~~**~~."~~

"1.6.2.2. **The interface type for the hose coupling shall be :**

 **a)** sealing cone of swivel-nut type of the type with a half vertical angle of 45°.

 **b) other couplings complying with the tests described in paragraph 1.7., as well as the tests mentioned in Annexes 5A and 5B.**

 **In case of an interface type using a soft seal body (e.g. O-ring), the type of material chosen shall be tested in accordance with Annexes 5D, 5F and 5G.”**

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_