|  |  |  |
| --- | --- | --- |
|   | United Nations | ECE/TRANS/WP.29/GRSP/2016/2 |
| _unlogo | **Economic and Social Council** | Distr.: General25 February 2016Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Passive Safety**

**Fifty-ninth session**

Geneva, 9-13 May 2016

Item 9 of the provisional agenda

**Regulation No. 16 (Safety-belts)**

 Proposal for the 07 series of amendments to Regulation
No. 16 (Safety-belts)

 Submitted by the experts from France Japan, Republic of Korea and European Commission[[1]](#footnote-2)\*

The text reproduced below was prepared by the experts from Japan, France, Republic of Korea and European Commission, aimed at introducing provisions on safety-belt reminders (SBRs) in all vehicle seats. It is based on informal document
GRSP-58-29-Rev.1 distributed at the fifty-eighth session of the Working Party on Passive Safety (GRSP). The modifications to the current text of UN Regulation No. 16 are marked in bold for new or strikethrough for deleted characters.

 I. Proposal

*Paragraph 1.4.,* amend to read and delete the footnote:

"1.4. **All seating positions in vehicle categories M and N fitted with safety belt with regard to safety belt reminder**

 ~~Vehicles of categories M~~~~1~~ ~~with regard to safety belt reminder[[2]](#footnote-3)2"~~

*Paragraph 2.41*.,amend to read:

"2.41. "*Safety-belt reminder*", means a system dedicated to alert the driver when ~~he/she~~ **any of the occupants** do not use the safety-belt. The system is constituted by a detection of an unfastened safety-belt and by two levels of driver's alert: a first level warning and a second level warning."

*Paragraphs 2.44. to 2.46*.,amend to read:

"2.44. "*First level warning*" means a visual warning activated when the ignition switch **or master control switch** is ~~engaged~~ **activated** ~~(engine running or not)~~ and ~~the driver's~~ **any of the occupants** safety-belt isnot fastened. An audible warning can be added as an option.

2.45. "*Second level warning*" means a visual and audible warning activated when ~~a driver operates a~~ **the** vehicle **is operated** without ~~fastening~~ the safety-belt **for any of the occupants being fastened**.

2.46. "*Safety-belt is not fastened*" means, at the option of the manufacturer, either the ~~driver~~ safety-belt buckle **of any occupant** is not engaged or the webbing length pulled out of the retractor is 100 mm or less."

*Paragraph 5.2.2.,* amend to read:

"5.2.2. An approval number shall be assigned to each type approved. Its first two digits (at present ~~06~~**07** corresponding to the ~~06~~**07** series of amendments) shall indicate the series of amendments …"

*Paragraphs 8.4.1.* *and* *8.4.1.1*., shall be deleted.

*Insert new paragraphs 8.4.1. to 8.4.1.3*., to read:

"**8.4.1. Requirements per specific seating position and exemptions**

**8.4.1.1. The seating position of the driver of M and NB categories of vehicles[[3]](#footnote-4)10 as well as the seating positions of the occupants of seats in the same row as the driver seat of M and N categories of vehicles shall be equipped with a safety-belt reminder satisfying the requirements of paragraph 8.4.2.**

**8.4.1.2. All seating positions of the rear seat row(s) of M1 and N1 category vehicles10 shall be equipped with a safety-belt reminder satisfying the requirements of paragraph 8.4.2.**

**Where the vehicle manufacturer provides a safety-belt reminder system on a rear seating position in another category of vehicle, the safety-belt reminder system may be approved according to this Regulation.**

**8.4.1.3. A safety-belt reminder is not compulsory on folding seats (i.e. normally folded and designed for occasional use) as well as seating positions fitted with an S-type belt or Harness belt and removable rear seats that have fully integrated safety belt.**

**Notwithstanding paragraph[s 8.4.1.1. and] 8.4.1.2 above, safety belt reminders are also not required in ambulances, vehicles used for transport of disabled persons, hearses as well as vehicles intended for use by the armed services, civil defence, fire services and forces responsible for maintaining public order.** "

*Paragraph 8.4.2.1.1.*, amend to read:

"8.4.2.1.1. Visual warning shall be so located as to be readily visible and recognisable in the daylight **and at night time** by the driver and distinguishable from other alerts. **For the seating positions defined in paragraph 8.4.1.1, the colour and symbol defined in** ~~Where the visual signal warning employs the colour red, it shall use a symbol in accordance with~~ item 21 in Table 1 of Regulation No. 121 **shall be used**.

~~(item K.01 – ISO 2575:2000) or, ~~"

*Paragraph 8.4.2.1.2*., amend to read:

"8.4.2.1.2. Visual warning shall be~~by continuous~~ **a** **steady** or ~~intermittent signal~~ **flashing tell-tale**."

*Insert a new paragraph* *8.4.2.1.3.*, to read:

"**8.4.2.1.3.** **A combined tell-tale may be used for safety-belts covered by paragraph 8.4.1.1.**

**However, for safety-belts covered by paragraph 8.4.1.2., the visual warning shall indicate all seating positions to allow the driver to identify, while facing forward as seated on the driver seat, any seating position in which the safety-belt is not fastened. The visual warning may contain different symbols than the one specified in paragraph 8.4.2.1.1. for safety-belts covered by paragraph 8.4.1.1.**"

*Paragraphs 8.4.2.1.3.,* renumber as 8.4.2.1.4.and amend to read:

"8.4.2.1.~~3.~~**4.** Audible warning shall be by a continuous or an intermittent**, though frequent,** sound signal orby **continuous** vocal information. Where vocal information is employed, the **vehicle** manufacturer shall ensure that the alert ~~uses~~ **is able to employ** the languagesof the market into which the vehicle is~~sold~~**intended to be used.** ~~This audible warning may be constituted by more than one step.~~ "

*Paragraph 8.4.2.2*., amend to read:

"8.4.2.2. **The** ~~F~~first level warning shall be at least a visual warning activated for ~~4~~**30** seconds or longer **for safety-belts covered by paragraph 8.4.1.1. and for 60 seconds or longer for safety-belts covered by paragraph 8.4.1.2.** when the ~~driver~~ safety-belt **of any of the seats** is not fastened and the ignition switch **or master control switch** is ~~engaged~~**activated**. **The first level warning may be cancelled by the driver for safety-belts covered by paragraph 8.4.1.2.**"

*Paragraph 8.4.2.4*., amend to read:

"8.4.2.4. Second level warning shall be a visual and audible signal activated for **at least** 30 seconds ~~or longer except for cases~~ **not counting periods** in which the warning **may** stop~~s~~ for ~~over~~**up to** 3seconds ~~when the safety-belt is not fastened, when the vehicle is in normal operation and when at least one of the following conditions (or any combination of these conditions),~~ **while one or all of the conditions set out in paragraphs 8.4.2.4.1. and 8.4.2.4.2.** is**/are** fulfilled**. The second level warning shall supersede the first level warning when the first level warning is still active.**"

*Paragraph 8.4.2.4.1.*, shall be deleted.

*Insert a new paragraph 8.4.2.4.1*., to read:

"**8.4.2.4.1.** **When a safety-belt covered by paragraph 8.4.1.1. is or becomes unfastened, for both scenarios, when the vehicle is in normal operation and under one or any combination of the conditions set out in paragraphs 8.4.2.4.2.1. to 8.4.2.4.2.4.**"

*Paragraphs 8.4.2.4.2. and 8.4.2.4.3.*, shall be deleted.

*Insert new paragraphs 8.4.2.4.2*. *to 8.4.2.4.2.4*., to read:

"**8.4.2.4.2. When a safety-belt covered by paragraph 8.4.1.2. becomes unfastened, when the vehicle is in normal operation and under one or any combination of the conditions set out in paragraphs 8.4.2.4.2.1. to 8.4.2.4.2.4.**

**8.4.2.4.2.1. The distance driven is greater than the distance threshold. The threshold shall not exceed 500 m. The distance driven when the vehicle is not in normal operation shall be excluded.**

**8.4.2.4.2.2. The vehicle speed is greater than the speed threshold. The threshold shall not exceed 25 km/h.**

**8.4.2.4.2.3. The duration time (engine running, propulsion system activated, etc.) is greater than the duration time threshold. The threshold shall not exceed 60 seconds. The first level warning duration time and the duration time when the vehicle is not in normal operation shall be excluded.**

**8.4.2.4.2.4. The thresholds to trigger safety belt reminder listed in paragraphs 8.4.2.4.2.1. to 8.4.2.4.2.3. above, may be reset when any of the doors have been opened at stand-still.**"

*Paragraph 8.4.2.6.1.*, amend to read:

"8.4.2.6.1. In the case that a short term deactivation isprovided, it shall be **significantly** more difficult to deactivate the safety-belt reminder than buckling the safety-belt on and off **(i.e. it shall consist of an operation of specific controls that are not integrated in the safety-belt buckle) and this operation shall only be possible when the vehicle is stationary**. When the ignition **or master control switch** is ~~switched off~~ **deactivated** for more than 30 minutes and ~~switched on~~ **activated** again, a short-term deactivated safety-belt reminder shall reactivate. **It shall not be possible to provide short term deactivation of the relevant visual warning(s).**"

*Insert new paragraphs 15.4. to 15.4.3.,* to read:

"**15.4. As from the official date of entry into force of the 07 series of amendments, no Contracting Party applying this Regulation shall refuse to grant approvals under this Regulation as amended by the 07 series of amendments.**

**15.4.1. As from 1 September [2018], Contracting Parties applying this Regulation shall grant type approvals only if the vehicle type to be approved meets the requirements of this Regulation as amended by the 07 series of amendments.**

**15.4.2.** **As from 1 September [2020], after the date of entry into force of the 07 series of amendments, Contracting Parties applying this Regulation may refuse to recognize approvals which were not granted in accordance with the 07 series of amendments to this Regulation.**

**15.4.3. Even after the date of entry into force of the 07 series of amendments, approvals of components and separate technical units in accordance with the preceding series of amendments to the Regulation shall remain valid and Contracting Parties applying the Regulation shall continue to accept them, and Contracting Parties may continue to grant extensions to the relevant component or separate technical unit approvals to the 06 series of amendments.**"

*Annex 2*, amend to read:

"Annex 2

 Arrangements of approval marks

1. Arrangements of the vehicle approval marks concerning the installation of safety-belts

Model A

(See paragraph 5.2.4. of this Regulation)



The above approval mark affixed to a vehicle shows that the vehicle type concerned has, with regard to safety-belts, been approved in the Netherlands (E 4) pursuant to Regulation No. 16. The approval number indicates that the approval was granted according to the requirements of Regulation No. 16 as amended by the **07** series of amendments.

Model B

(See paragraph 5.2.5. of this Regulation)

****

The above approval mark affixed to a vehicle shows that the vehicle type concerned has been approved in the Netherlands (E 4) pursuant to Regulations Nos. 16 and 52.[[4]](#footnote-5) The approval numbers indicate that, at the dates when the respective approvals were given, Regulation No. 16 included the **07** series of amendments and Regulation No. 52 the 01 series of amendments.

…"

*Annex 18,*

 *Paragraph 1*, amend to read:

"1. The first level warning shall be tested according to the following conditions:

 (a) Safety-belt is not fastened;

(b) Engine **or propulsion system** is stopped or idling**,** and the vehicle is not in forward or reverse motion;

 (c) Transmission is in neutral position;

 (d) Ignition switch **or master control switch** is ~~engaged~~**activated**.

**(e) A load of 40 kg is placed on each seat cushion in the same row as the driver's seat, or the simulated state in which occupants are on-board the vehicle by an alternative method specified by the vehicle manufacturer, provided an occupant’s load does not exceed 40 kg. This may also be done for the rear seats at the request of the vehicle manufacturer.**"

*Paragraph 2.,* amend to read:

"2. The second level warning shall be tested according to the ~~following~~ conditions **set out in paragraphs 2.1. to 2.3. of this Annex, respectively.**

 ~~(a) Safety-belt is not fastened;~~

~~(b) Test vehicle driven with one or any combination of the conditions of paragraphs 2.1. to 2.3. of this annex at the manufacturer's choice.~~"

*Paragraphs 2.1. to 2.3.*, shall be deleted.

*Insert new paragraphs 2.1. to 2.3.*, to read:

"**2.1. Testing the driver's seating position**

**2.1.1. Testing the driver’s seat when the safety-belt is unfastened before the journey**

**(a) The safety-belt of the driver's seat is not fastened;**

**(b) The safety-belts of seats other than the driver's seat are fastened;**

**(c) Test vehicle driven with one or any combination of the conditions of paragraphs 2.1.1.1. to 2.1.1.3. of this annex at the manufacturer's choice.**

**2.1.1.1. Accelerate the test vehicle to 25 -0/+10 km/h from a halt and continue on the same speed.**

**2.1.1.2. The test vehicle is driven forward at least 500 m from a halt position.**

**2.1.1.3. The vehicle is tested when the vehicle is in normal operation for at least 60 seconds.**

**2.1.2. Testing the driver’s seat when the safety-belt becomes unbuckled during the journey.**

**(a) The safety-belts of the driver’s seat and seats other than the driver’s seat are fastened.**

**(b) The test vehicle is driven, at the choice of the manufacturer, under one of the conditions in paragraphs 2.1.1.1. to 2.1.1.3. of this annex or a combination thereof;**

**(c) The safety-belt of the driver’s seat is unbuckled.**

**2.2. Testing the seating position(s) in the same row as the driver's seat**

**2.2.1.** **Testing the seat(s) in the same row as the driver's seat when the safety-belt is unfastened before the journey:**

**(a) The safety-belt(s) of the seat(s) in the same row as the driver's seat is/are not fastened;**

**(b) The safety-belts of the seats other than the seat(s) in the same row as the driver's seat are fastened;**

**(c) A load of 40 kg is applied to the seat(s) in the same row as the driver's seat, or the state in which occupants are on-board the vehicle is simulated by a method specified by the manufacturer;**

**(d) The test vehicle is driven, at the choice of the manufacturer, under one of the conditions in paragraphs 2.1.1.1. to 2.1.1.3. of this annex or combination thereof;**

**(e) The state of the safety-belt reminder is checked for all of the seat(s) in the same row as the driver's seat, in conditions (a) to (d).**

**2.2.2. Testing the seating position in the same row as the driver’s seat when the safety-belt becomes unbuckled during the journey.**

**(a) The safety-belts of the driver’s seat and seats other than the driver’s seat are fastened;**

**(b) A load of 40 kg is applied to the seat(s) in the same row as the driver's seat, or the state in which occupants are on-board the vehicle is simulated by a method specified by the manufacturer;**

**(c) The test vehicle is driven, at the choice of the manufacturer, under one of the conditions in paragraphs 2.1.1.1. to 2.1.1.3. of this annex or combination thereof;**

**(d) The safety-belt of the seats other than the seat(s) in the same row as the driver's seat is unbuckled.**

**(e) The state of the safety-belt reminder is checked for all of the seat(s) in the same row as the driver's seat, for each condition (a) to (d).**

**2.3. Testing the rear seats**

**(a) With the test vehicle stationary, the safety-belts of all seats are fastened;**

**(b) The test vehicle is put in normal operation and kept running;**

**(c) The safety-belt of one of the rear seats is unfastened;**

**(d) The functioning of the safety-belt reminder is checked for all of the seating positions in all seating rows;**

**(e) Alternatively, at the request of the vehicle manufacturer, the test procedures specified in paragraphs 2.2. to 2.2.2. for the seating position(s) in the same row as the driver's seat may be used for any rear seating position instead.**"

*Paragraph 3*, amend to read:

"3. **The first level warning test shall have a duration of at least the minimum required time as specified in paragraph 8.4.2.2. of this Regulation for the first level warning. The second level warning test may be initiated after completion of the first level warning test. However, it shall also be ensured that the second level warning supersedes the first level warning when the first level warning is still active**."

 II. Justification

1. It is widely recognised that the safety-belt is one of the most important and effective vehicle safety features.

2. Nevertheless, actual safety-belt wearing rates vary greatly between countries and also differ between front and rear seating positions, as was explained in a presentation provided at the fifty-seventh session of GRSP.

3. In Japan, rear seat safety-belt use can be as low as 35.1 per cent.

4. When the effective SBR is mandatory for all passenger car seats, an expected 150 lives can be saved annually in Japan.

5. In the Republic of Korea, seat safety-belt use is generally between 80 per cent and 90 per cent on front seats, but even as low as 16.2 per cent on rear seats.

6. In 2013, three hundred people not wearing a safety-belt died in cars in the Republic of Korea, and over 18,000 persons not wearing safety-belts were injured. When the fitment of SBR will be mandatory for all passenger car seats in the Republic of Korea, 103 lives are expected to be saved in target year 2024 with a 70 per cent observance rate of the SBR. In the same condition, the cost-benefit ratio will be 1.43.

7. The European Commission published a study that quantifies the casualty benefit of legislative action on SBRs for all M and N categories of vehicles by comparing a baseline, i.e. "do nothing" scenario, with an action scenario which involved mandating SBRs. The relevant findings, including Benefit-to-Cost ratios, can be found in the report available at:

<http://ec.europa.eu/DocsRoom/documents/6662/attachments/1/translations/en/renditions/pdf>

8. Through our analysis described above, we could recognize the effectiveness of SBR. At the same time, we recognized the importance of other measures than SBR, such as police enforcement, driver education, and promotion through media. So, such measures are expected to be continued in order to enhance the safety belt wearing rates further together with this amendment for SBR.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2014–2018 (ECE/TRANS/240, para. 105 and ECE/TRANS/2014/26, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)
2. ~~2 Japan shall not be prevented, by the obligations of the Agreement to which this Regulation is annexed, from requiring vehicles of category N~~~~1~~~~, which are granted type-approvals under this regulation to meet its existing national requirements for safety-belt reminders.~~ [↑](#footnote-ref-3)
3. 10 As defined in the Consolidated Resolution on the Construction of Vehicles (R.E.3.), document ECE/TRANS/WP.29/78/Rev.4, para. 2 - [www.unece.org/trans/main/wp29/wp29wgs/wp29gen/wp29resolutions.html](http://www.unece.org/trans/main/wp29/wp29wgs/wp29gen/wp29resolutions.html) [↑](#footnote-ref-4)
4. The second number is given merely as an example. [↑](#footnote-ref-5)