|  |
| --- |
| **UN/SCETDG/52/INF.56** |
| **Committee of Experts on the Transport of Dangerous Goods and on the Globally Harmonized System of Classification and Labelling of Chemicals**  **Sub-Committee of Experts on the Transport of Dangerous Goods 30 November 2017**  **Fifty-second session**  Geneva, 27 November-6 December 2017  Item 7 of the provisional agenda **Global harmonization of transport of dangerous goods  regulations with the Model Regulations** |

Name and description of UN 3363 –Revision of 2017/34

Transmitted by the expert from Germany

Proposal

DANGEROUS GOODS IN ARTICLES or DANGEROUS GOODS IN MACHINERY or DANGEROUS GOODS IN APPARATUS

Amend SP 301 as follows:

“This entry only applies to articles such as machinery, apparatus or devices containing dangerous goods as a residue or an integral element of the article. It shall not be used articles for which a proper shipping name already exists in the Dangerous Goods List of Chapter 3.2. Articles transported under this entry shall only contain dangerous goods which are authorized to be transported in accordance with the provisions of Chapter 3.4 (Limited quantities). The quantity of dangerous goods in articles shall not exceed the quantity specified in Column 7a of the Dangerous Goods List of Chapter 3.2 for each item of dangerous goods contained. If the article contains more than one item of dangerous goods, the individual substances shall be enclosed to prevent them reacting dangerously with one another (see 4.1.1.6).When it is required to ensure liquid dangerous goods remain in their intended orientation, package orientation labels meeting the specifications of ISO 780:1997 shall be affixed on at least two opposite vertical sides with the arrows pointing in the correct direction.

The competent authority may exempt from regulation articles which would otherwise be transported under this entry.