|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.15/AC.1/2017/23 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  2 June 2017  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods**

Geneva, 19-29 September 2017

Item 6 of the provisional agenda

**Interpretation of RID/ADR/ADN**

Interpretation of RID/ADR 7.5.1.2 and ADR 7.5.1.1: “Equipment used”

Transmitted by the Government of Germany[[1]](#footnote-2), [[2]](#footnote-3)\*\*

1. The end of the second indent of RID/ADR, 7.5.1.2 refers to the visual inspection of the “... equipment used in loading and unloading...”. This wording is also to be found in ADR 7.5.1.1 in connection with arrival at the loading and unloading sites.

2. In Germany, there has been uncertainty as to what equipment has to be inspected. In particular, the question is whether this reference also includes all the equipment in accordance with ADR 8.1.4 and 8.1.5, as well as the personal protective equipment in accordance with the instructions in writing of RID/ADR Chapter 5.4. Opinions differ particularly in terms of the loader’s inspection of the fire extinguishers before loading or unloading. However, it would seem reasonable to include these pieces of equipment, because they might also be used in the event of incidents during loading work.

3. The Government of Germany requests the Joint Meeting for its view on the above.

1. In accordance with the programme of work of the Inland Transport Committee for 2016-2017, (ECE/TRANS/2016/28/Add.1 (9.2)). [↑](#footnote-ref-2)
2. \*\* Circulated by the Intergovernmental Organisation for International Carriage by Rail (OTIF) under the symbol OTIF/RID/RC/2016/23. [↑](#footnote-ref-3)