|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2017/40 |
| Description: _unlogo | **Economic and Social Council** | Distr.: General20 December 2016Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**171st session**

Geneva, 14-17 March 2017

Item 4.9.22 of the provisional agenda

**1958 Agreement:**

**Consideration of draft amendments**

**to existing Regulations submitted by GRE**

Proposal for Supplement 5 to the 01 series of amendments to Regulation No. 119 (Cornering lamps)

**Submitted by the Working Party on Lighting and Light-Signalling**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Lighting and Light-Signalling (GRE) at its seventy-sixth session (ECE/TRANS/WP.29/GRE/76, paras. 10, 13, 14 and 31). It is based on ECE/TRANS/WP.29/2013/94, ECE/TRANS/WP.29/GRE/2013/55/Rev.1, ECE/TRANS/WP.29/GRE/2014/3, ECE/TRANS/WP.29/GRE/2016/27, ECE/TRANS/WP.29/GRE/2016/30, ECE/TRANS/WP.29/GRE/2016/31 and Annex II to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their March 2017 sessions.

Supplement 5 to the 01 series of amendments to Regulation No. 119 (Cornering lamps)

*Paragraph 1.2.1.,* amend to read:

"1.2.1. The trade name or mark:

(a) Lamps bearing the same trade name or mark but produced by different manufacturers shall be considered as being of different types;

(b) Lamps produced by the same manufacturer differing only by the trade name or mark shall be considered as being of the same type."

*Insert a new paragraph 2.2.4.,* to read:

"2.2.4. In the case of a type of lamp differing only by the trade name or mark from a type that has already been approved it shall be sufficient to submit:

2.2.4.1. A declaration by the lamp manufacturer that the type submitted is identical (except in the trade name or mark) with and has been produced by the same manufacturer as, the type already approved, the latter being identified by its approval code;

2.2.4.2. Two samples bearing the new trade name or mark or equivalent documentation."

*Insert a new paragraph 2.2.5.*, to read:

"2.2.5. In the case of a non-replaceable filament lamp(s) or light source module(s) equipped with non-replaceable filament lamp(s), the documents according to paragraph 5.5. of this Regulation."

*Paragraph 3.,* amend to read:

"3. Markings

 Cornering lamps submitted for approval shall:

3.1. Bear………………"

*Paragraph 3.4.,* amend to read:

"3.4. In the case of lamps with an electronic light source control gear and/or non replaceable light sources and/or light source module(s), bear the marking of the rated voltage or range of voltage."

*Paragraph 3.5.3.,* amend to read:

"3.5.3. The marking of the rated voltage or range of voltage."

*Paragraph 5.*, amend to read:

**"5. General specifications**

 The requirements contained in sections 5. "General specifications" and 6. "Individual specifications" and in the Annexes referenced in the said sections of Regulations Nos. 48 or 86, and their series of amendments in force at the time of application for the lamp type approval shall apply to this Regulation.

 The requirements pertinent to each lamp and to the category/ies of vehicle on which the lamp is intended to be installed shall be applied, where its verification at the moment of lamp type approval is feasible.

5.1. …"

*Insert a new paragraph 5.5.*, to read:

"5.5. In the case of non-replaceable filament lamp(s) or light source module(s) equipped with non-replaceable filament lamp(s), the applicant shall annex to the type approval documentation a report (by the light source manufacturer indicated in the type approval documentation), acceptable to the Authority responsible for type approval, that demonstrates compliance of these non‑replaceable filament lamp(s) with the requirements as specified in paragraph 4.11. of IEC 60809, Edition 3."

*Paragraph 6.4.*amend to read:

"6.4. In the case of a single lamp containing more than one light source when all light sources are illuminated the maximum intensities shall not be exceeded."

*Insert a new paragraph 6.5.* to read:

"6.5. Failure of a single lamp containing more than one light source:

6.5.1. In a single lamp containing more than one light source, a group of light sources, wired so that the failure of any one of them causes all of them to stop emitting light, shall be considered to be one light source.

6.5.2. In case of failure of any one light source in a single lamp containing more than one light source, at least one of the following provisions shall apply:

 (a) The light intensity complies with the minimum intensity required in the table of standard light distribution in space as shown in Annex 3, or

 (b) A signal for activation of a tell-tale indicating failure, as indicated in paragraph 6.20.8. of Regulation No. 48, is produced, provided that the luminous intensity at 2.5°D 45°L for a left-side lamp (the L angle should be substituted for the R angle for a right-side lamp) is at least 50 per cent of the minimum intensity required. In this case a note in the communication form states that the lamp is only for use on a vehicle fitted with a tell-tale indicating failure."

*Paragragh 7.5.,* shall bedeleted.

*Paragraph 9.1,* amend to read:

"9.1. Cornering lamps shall be so manufactured as to conform to the corresponding type approved according to this Regulation.

The compliance with the requirements set forth in paragraphs 6. and 8. above shall be verified as follows:"

*Paragraph 9.2. (former)*, renumber as paragraph 9.1.1.

*Paragraph 9.3. (former)*, renumber as paragraph 9.1.2.

*Paragraph 9.4. (former)*, renumber as paragraph 9.2.

*Insert a new paragraph 9.3.,* to read:

"9.3. In the case of non-replaceable filament lamp(s) or light source module(s) equipped with non-replaceable filament lamps, a report (by the light source manufacturer indicated in the type approval documentation) shall demonstrate compliance of these non-replaceable filament lamp(s) with lifetime requirements and, in the case of colour coated filament lamps, also with colour endurance requirements, as specified in paragraph 4.11. of IEC 60809, Edition 3."

*Annex 1,*

*Item 9*, amend to read:

"9. Concise description:

 By category of lamp:

 Number, category and kind of light source(s):2

 Voltage and wattage:

 Light source module: yes/no3

 Light source module specific identification code:

 Application of an electronic light source control gear:

(a) Being part of the lamp: yes/no3

(b) Being not part of the lamp: yes/no3

 Input voltage supplied by an electronic light source control gear:

 Electronic light source control gear manufacturer and identification number (when the light source control gear is part of the lamp but is not included into the lamp body):

 Geometrical conditions of installation and relating variations, if any:

 The lamp is only for use on a vehicle fitted with a tell-tale indicating failure: yes/no3"

*Annex 5,*

*Insert new paragraphs 1.4. to 1.4.2.*, to read:

"1.4. In the case of non-replaceable filament lamp(s) or light source module(s) equipped with non-replaceable filament lamps, at any conformity of production check:

1.4.1. The holder of the approval mark shall demonstrate the use in normal production and show the identification of the non-replaceable filament lamp(s) as indicated in the type approval documentation;

1.4.2. In the case where doubt exists in respect to compliance of the
non-replaceable filament lamp(s) with lifetime requirements and/or, in the case of colour coated filament lamps, with colour endurance requirements, as specified in paragraph 4.11 of IEC 60809, Edition 3, conformity shall be checked (by the light source manufacturer indicated in the type approval documentation) as specified in paragraph 4.11. of IEC 60809, Edition 3."

*Annex 6,*

*Paragraphs 2 to 5*, amend to read:

"2. First sampling

In the first sampling four cornering lamps are selected at random. The first sample of two is marked A, the second sample of two is marked B.

2.1. The conformity of mass-produced cornering lamps shall not be contested if the deviation of any specimen of samples A and B (all four lamps) is not more than 20 per cent.

In the case, that the deviation of both lamps of sample A is not more than 0 per cent, the measurement can be closed.

2.2. The conformity of mass-produced cornering lamps shall be contested if the deviation of at least one specimen of samples A or B is more than 20 per cent.

The manufacturer shall be requested to bring his production in line with the requirements (alignment) and a repeated sampling according to paragraph 3. below shall be carried out within two months' time after the notification. The samples A and B shall be retained by the Technical Service until the entire Conformity of Production process is finished.

3. First repeated sampling

A sample of four lamps is selected at random from stock manufactured after alignment.

The first sample of two is marked C, the second sample of two is marked D.

3.1. The conformity of mass-produced cornering lamps shall not be contested if the deviation of any specimen of samples C and D (all four lamps) is not more than 20 per cent.

In the case, that the deviation of both lamps of sample C is not more than 0 per cent the measurement can be closed.

3.2. The conformity of mass-produced cornering lamps shall be contested if the deviation of at least:

3.2.1. One specimen of samples C or D is more than 20 per cent but the deviation of all specimen of these samples is not more than 30 per cent.

The manufacturer shall be requested again to bring his production in line with the requirements (alignment).

A second repeated sampling according to paragraph 4. below shall be carried out within two months' time after the notification. The samples C and D shall be retained by the Technical Service until the entire Conformity of Production process is finished.

3.2.2. One specimen of samples C and D is more than 30 per cent.

In this case the approval shall be withdrawn and paragraph 5. below shall be applied.

4. Second repeated sampling

A sample of four lamps is selected at random from stock manufactured after alignment.

The first sample of two is marked E, the second sample of two is marked F.

4.1. The conformity of mass-produced cornering lamps shall not be contested if the deviation of any specimen of samples E and F (all four lamps) is not more than 20 per cent

In the case, that the deviation of both lamps of sample E is not more than 0 per cent, the measurement can be closed.

4.2. The conformity of mass-produced cornering lamps shall be contested if the deviation of at least one specimen of samples E or F is more than 20 per cent.

In this case the approval shall be withdrawn and paragraph 5. below shall be applied.

5. Approval withdrawn

Approval shall be withdrawn according to paragraph 10. of this Regulation."

*Figure 1*, shall be deleted.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)