**Comment on document ECE/TRANS/WP.29/GRSG/2017/15** - Proposal for Supplement 7 to the 01 series of amendments to Regulation No. 43 (Safety glazing)

(Addition to existing text of ECE/TRANS/WP.29/GRSG/2017/15 is shown in bold italic text and deletion in double strikethrough and highlighting all modifications)

**I. Proposal**

*Annex 21* ***Annex 18****, Table 2,* amend to read:

"

| *Seat-back angle*  *(in °)* | *Horizontal  co-ordinates*  *X* | *Vertical  co-ordinates*  *Z* | *Seat-back angle*  *(in °)* | *Horizontal co-ordinates*  *X* | *Vertical co-ordinates*  *Z* |
| --- | --- | --- | --- | --- | --- |
| 5  6  7  8  9  10  11  12  13  14  15  16  17  18  19  20  21  22 | - 186 mm  ***- 177 mm*** - 176mm  - 167 mm  - 157 mm  - 147 mm  - 137 mm  - 128 mm  - 118 mm  - 109 mm  - 99 mm  - 90 mm  - 81 mm  ***- 72 mm*** - 71 mm  - 62 mm  - 53 mm  - 44 mm  - 35 mm  - 26 mm | 28 mm  27 mm  27 mm  ***27 mm*** 26 mm  26 mm  25 mm  24 mm  23 mm  22 mm  21 mm  20 mm  18 mm  17 mm  15 mm  13 mm  11 mm  9 mm  7 mm | 23  24  25  26  27  28  29  30  31  32  33  34  35  36  37  38  39  40 | - ~~17~~ **18** mm  - 9 mm  0 mm  9 mm  17 mm  26 mm  34 mm  43 mm  51 mm  59 mm  67 mm  76 mm  84 mm  92 mm  100 mm  ~~107~~ **108** mm  115 mm  123 mm | 5 mm  ~~2~~ **3** mm  0 mm  - 3 mm  - 5 mm  - 8 mm  - 11 mm  - 14 mm  - 17 mm  - 21 mm  - 24 mm  - 28 mm  - 31 mm  - 35 mm  - 39 mm  - 43 mm  - ~~47~~ **48** mm  - 52 mm |

"

**II. Justification for comments**

When proposal is compared with corresponding Table 2 of UN GTR No. 6, highlighted mismatch were found.

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_