|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2018/21 |
| Description: _unlogo | **Economic and Social Council** | Distr.: General28 December 2017Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**174th session**

Geneva, 13-16 March 2018

Item 4.8.7 of the provisional agenda

**1958 Agreement:
Consideration of draft amendments**

**to existing UN Regulations submitted by GRSG**

Proposal for the 08 series of amendments to UN Regulation No. 107 (M2 and M3 vehicles)

**Submitted by the Working Party on General Safety Provisions**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on General Safety Provisions (GRSG) at its 113th session (ECE/TRANS/WP.29/GRSG/92, paras. 5 and 6). It is based on official documents ECE/TRANS/WP.29/GRSG/2016/20 and ECE/TRANS/WP.29/GRSG/2017/14 as reproduced in Annex V to the report. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their March 2018 sessions.

*List of contents*, amend to read:

"Annex 5 Requirements to establish the visual contrast"

*Insert new paragraphs 2.44. to 2.48. (Definitions)*, to read:

"2.44. *"Visual contrast"* (luminance contrast) means the brightness ratio between an object and its immediate background/surrounding which allows the object to be distinguished from its background/surroundings.

2.45. *"Reflectance"* ρ (rho) is the quantitative ratio between reflected light and the incident light on the surface of a flat material. It consists of various portions of "regular reflectance" and "diffuse reflectance".

2.46. *"Regular reflectance"* ρr is the reflection without diffusion in accordance with the laws of optical reflection as in a mirror.

2.47. *"Diffuse reflectance"* ρd is the ratio of the light that has undergone diffuse reflection to the incident light.

2.48. *"Luminous flux"* Φ (phi) describes the power of a light source."

*Insert new paragraphs 10.19. to 10.23.*, to read:

"10.19. As from the official date of entry into force of the 08 series of amendments, no Contracting Party applying this Regulation shall refuse to grant or refuse to accept UN type-approvals under this Regulation as amended by the 08 series of amendments.

10.20. As from 1 September 2020, Contracting Parties applying this Regulation shall not be obliged to accept UN type-approvals to the preceding series of amendments, first issued after 1 September 2020.

10.21. Until 1 September 2022, Contracting Parties applying this Regulation shall accept UN type-approvals to the preceding series of amendments, first issued before 1 September 2020.

10.22. As from 1 September 2022, Contracting Parties applying this Regulation shall not be obliged to accept type-approvals issued to the preceding series of amendments to this Regulation.

10.23. Contracting Parties applying this Regulation shall not refuse to grant UN type-approvals according to any preceding series of amendments to this Regulation or extensions thereof."

*Annex 3*

*Paragraph 7.11.4.,* amend to read:

"7.11.4. Handrails and handholds in toilets."

*Insert new paragraph 7.11.4.1.*, to read:

"7.11.4.1. If a toilet is fitted, a suitable handrail or handhold shall be provided in the interior."

*Annex 5,* amend to read:

"**Annex 5**

 **Requirements to establish the visual contrast per paragraph 3.3.3. of Annex 8**

1. The visual contrast C shall be established according to the following formula:

 With: ρ1 = the reflectance of the material of the object to be seen

 ρ2 = the reflectance of the area respectively material surrounding the contrast object

2. For determination of the reflectance values ρ1, ρ2 and ρd an integrating sphere according to CIE 38:1977 shall be used.

 The reflectance shall be either read directly from the indicating instrument or calculated according to the following formula:

 Where:

 Φ1 = luminous flux of the incident light on the material sample;

 Φ2 = luminous flux of the reflected light (reflectance).

2.1. The illumination angle of the luminous flux of the incident light on the sample Θi shall be equal to 8° ± 0.5°.

2.2. The luminous flux of the incident light on the sample shall be determined by using a diffuse reflectance standard calibrated by an accredited laboratory. The extended measurement uncertainty shall be lower than 3 per cent.

3. Example of an integrating sphere according to CIE 38:1977:

"

*Annex 8*

*Paragraph 3.3.3.*, amend to read:

"3.3.3. These communication devices shall:

3.3.3.1. provide either a visual contrast of C ≥ 0.4 and a diffuse reflectance ρd of at least 0.5 according to Annex 5 or be white or yellow,

3.3.3.2. provide a tactile surface, i.e. protrude from the surrounding areas,

3.3.3.3. provide an audible and visible signal to confirm successful activation."

*Paragraph 3.5.,* amend to read:

"3.5. Floor slope

 The slope of any gangway, access passage or floor area between any priority seat and at least one entrance and one exit or a combined entrance and exit shall not exceed 8 per cent. The slope of any gangway, access passage or floor area between any wheelchair space and at least one entrance and one exit or a combined entrance and exit shall not exceed 5 per cent. Such sloping areas shall be provided with a slip-resistant surface. However, in the gangway, access passages or floor area where differently directed slopes merge, these limits may be exceeded provided the total amount of these areas is not greater than 25 per cent of the total amount of the area swept by the wheelchair to reach the wheelchair area."

*Paragraph 3.6.1.*, amend to read:

"3.6.1. For each wheelchair user provided for in the passenger compartment there shall be a special area at least 750 mm wide and 1,300 mm long and 1,400 mm high. The longitudinal plane of the special area shall be parallel to the longitudinal plane of the vehicle and the floor surface of the special area shall be slip resistant and the maximum slope in ~~any~~ forward and rearward direction shall not exceed 5 per cent. In the lateral direction the slope shall not exceed 3 per cent. However, at the rear end of the wheelchair area where differently directed slopes merge, these limits may be exceeded provided the total amount of these areas is not greater than 25 per cent of the wheelchair area. Furthermore, in the case of a rearward facing wheelchair complying with the requirements specified in paragraph 3.8.4., the slope in the longitudinal direction shall not exceed 8 per cent provided that this slope inclines upwards from the front end to the rear end of the special area.

 In the case of a wheelchair space … as shown in Annex 4, Figure 22."

*Annex 12, paragraph 3.10.12.,* amend to read:

"3.10.12. Each of the insulations …

 … AC value.

 Circuits directly connected to overhead line shall be double insulated."

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update UN regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)