|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/2018/50 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  5 April 2018  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**175th session**

Geneva, 19-22 June 2018

Item 4.7.5 of the provisional agenda

**1958 Agreement:  
Consideration of draft amendments**

**to existing UN Regulations submitted by GRPE**

Proposal for Supplement 8 to UN Regulation No. 85 (Measurement of the net power)

**Submitted by the Working Party on Pollution and Energy**[[1]](#footnote-2)\*

The text reproduced below was adopted by the Working Party on Pollution and Energy (GRPE) at its seventy-sixth session (ECE/TRANS/WP.29/GRPE/76, para. 29). It is based on ECE/TRANS/WP.29/GRPE/2018/5, as amended by Annex VII of ECE/TRANS/WP.29/GRPE/76. It is submitted to the World Forum for Harmonization of Vehicle Regulations (WP.29) and to the Administrative Committee AC.1 for consideration at their June 2018 sessions.

Supplement 8 to UN Regulation No. 85 (Measurement of the net power)

*Paragraph 5.3.1.3.,* amend to read:

"5.3.1.3. Immediately prior to the test, the motor shall be run on the bench for three minutes delivering a power equal to either 80 per cent of the maximum 30 minutes power or 80 per cent of the maximum peak power at a speed recommended by the manufacturer, within the speed range determined in paragraph 5.3.2.2. Following the completion of this run, the power test shall be started within a maximum of 1 minute."

*Annex 5*

*Paragraph 5.4.2.,* amend to read:

"5.4.2. Diesel engines - Factor αd

The power correction factor (αd) for diesel engines at constant fuel rate is obtained by applying the formula:

Where αd = (fa) fm

fa is the atmospheric factor

fm is the characteristic parameter for each type of engine and adjustment"

1. \* In accordance with the programme of work of the Inland Transport Committee for 2018–2019 (ECE/TRANS/274, para. 123 and ECE/TRANS/2018/21, Cluster 3.1), the World Forum will develop, harmonize and update UN Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)