|  |  |
| --- | --- |
| Submitted by the expert from the Russian Federation | Informal document **GRSG-114-17**(114th GRSG, 9-13 April 2018agenda item 9) |

**Proposal for a Corrigendum to UN Regulation № 121
(Identification of controls, tell-tales and indicators)**

The text reproduced below was prepared by the expert from the Russian Federation with the aim of aligning the English and Russian texts of UN Regulation № 121. The proposal refers only the Russian text.

The modifications to Regulation № 121 are marked in bold for new characters and strikethrough for deleted characters.

**Corrigendum**

*Paragraphs 2.4 and 5.5.1.4*, correct to read:

*Пункт 2.4* изменить следующим образом:

"2.4 «Общее пространство» означает участок, на котором могут отображаться, но не ~~совмещаться~~ **одновременно**, не менее двух информационных функций (например, условных обозначений). "

*Пункт 5.5.1.4* изменить следующим образом:

"5.5.1.4 если контрольный сигнал, указывающий на неисправность тормозной системы, ~~или контрольные сигналы~~ дальнего света, указателей поворота или ремней безопасности~~,~~ отобража~~ю~~**е**тся в каком-либо общем пространстве, то **он** **должен замещать любое другое условное обозначение в данном общем пространстве,** в случае возникновения базового условия для ~~их~~ **его** включения~~, яркость этих сигналов должна значительно превышать яркость любого другого условного обозначения в таком общем пространстве~~;"

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_