**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**108th session 4 March 2020**

Geneva, 11–15 May 2020

Item 8 of the provisional agenda

**Any other business**

 Consequential amendments to Table B

 Note by the secretariat

 Purpose

Document ECE/TRANS/WP.15/249 has been published containing a consolidated list of all the amendments which the Working Party on the Transport of Dangerous Goods has adopted for entry into force on 1 January 2021. This document does not cover amendments to Table B in Chapter 3.2, as it does not form an integral part of ADR. The amendments necessary to bring Table B up to date with the changes made in Table A, already adopted at the previous session on the basis on informal document INF.7, are reproduced below.

 Proposal

 Chapter 3.2, Table B

Add the following new entries in proper order:

|  |  |  |
| --- | --- | --- |
| DETONATORS, ELECTRONIC programmable for blasting | 051105120513 | 111 |
| MEDICAL WASTE, CATEGORY A, AFFECTING HUMANS, solid | 3549 | 6.2 |
| MEDICAL WASTE, CATEGORY A, AFFECTING ANIMALS only, solid | 3549 | 6.2 |

Replace the entry for “DANGEROUS GOODS IN MACHINERY OR DANGEROUS GOODS IN APPARATUS” by the following 3 entries:

|  |  |  |
| --- | --- | --- |
| DANGEROUS GOODS IN APPARATUS | 3363 | 9 |
| DANGEROUS GOODS IN ARTICLES | 3363 | 9 |
| DANGEROUS GOODS IN MACHINERY | 3363 | 9 |

Amend the entry for “BUTADIENES AND HYDROCARBON MIXTURE, STABILIZED, having a vapour pressure at 70 °C not exceeding 1.1 MPa (11 bar) and a density at 50 °C not lower than 0.525 kg/l” to read “BUTADIENES AND HYDROCARBON MIXTURE, STABILIZED, containing more than 40% butadienes”.

Amend the entry for “2-DIMETHYLAMINOETHYL METHACRYLATE” to read “2-DIMETHYLAMINOETHYL METHACRYLATE, STABILIZED”.

Amend the entry for “MIXTURES OF 1,3-BUTADIENE AND HYDROCARBONS, STABILIZED, having a vapour pressure at 70 °C not exceeding 1.1 MPa (11 bar) and a density at 50 °C not lower than 0.525 kg/l” to read MIXTURES OF 1,3-BUTADIENE AND HYDROCARBONS, STABILIZED, containing more than 40% butadienes”.

Amend the entry for “RADIOACTIVE MATERIAL, LOW SPECIFIC ACTIVITY, (LSA-III), FISSILE” to read “RADIOACTIVE MATERIAL, LOW SPECIFIC ACTIVITY (LSA-III), FISSILE”.

Amend the entry for “RADIOACTIVE MATERIAL, SURFACE CONTAMINATED OBJECTS (SCO-I or SCO-II), non fissile or fissile-excepted” to read “RADIOACTIVE MATERIAL, SURFACE CONTAMINATED OBJECTS (SCO-I, SCO-II or SCO-III), non fissile or fissile-excepted”.