Proposal to correct the text of 00 series of Amendments to UN Regulation No. 149.

The modifications to the existing text are marked in bold for new or strikethrough for deleted characters.

1. Proposal

*Paragraph 4.13.,* amend to read:

“4.13. If applicable, the lamp shall be so made that, **if a light source and/or a LED module has faile**d, a failure signal in order to comply with the relevant provisions of UN Regulation No. 48 is provided.”

1. **Justification:**

1. The correction proposed, by the text added in paragraph 4.13., is done to correctly reflect the existing text of UN Regulation No. 123 concerning adaptive front-lighting systems (AFS). In current paragraph 4.13 for the provision of failure signal of UN Regulation No. 149, specific requirement of paragraph 5.9 in UN Regulation No. 123 for detection of failure of a light source and/or a LED module of AFS is missing.

2. This amendment is needed in order to align requirements of original series of UN Regulation No. 149 for Road Illumination Devices with current UN regulations for Lighting and Light-Signalling Devices, as agreed during 82nd session of GRE (paragraph 14. of the report, ECE/TRANS/WP.29/GRE/82)