|  |  |  |
| --- | --- | --- |
|  | E/ECE/324/Rev.1/Add.15/Rev.8/Corr.1−E/ECE/TRANS/505/Rev.1/Add.15/Rev.8/Corr.1 | |
|  |  | 12 February 2016 |

Agreement

Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

Addendum 15 – Regulation No. 16

Revision 8 – Corrigendum 1

Corrigendum 1 to Revision 8 of the Regulation *(Erratum by the secretariat)*

**Uniform provisions concerning the approval of:  
I. Safety-belts, restraint systems, child restraint systems and ISOFIX child restraint systems for occupants of power-driven vehicles  
II. Vehicles equipped with safety-belts, safety-belt reminders, restraint systems, child restraint systems and ISOFIX child restraint systems and i-Size child restraint systems**

**\_\_\_\_\_\_\_\_\_**



**UNITED NATIONS**

*Annex 16, the table,* correct to read:

E/ECE/324/Rev.1/Add.15/Rev.8/Corr.1  
E/ECE/TRANS/505/Rev.1/Add.15/Rev.8/Corr.1

| **Annex 16**  Safety-belt installation showing the belt types and retractor types | | | | | | | | | |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *Minimum requirements for safety-belts and retractors* | | | | | | | | | |
| *Vehicle category* | *Forward facing seating positions* | | | | | | *Rearward-facing*  *seating positions* | | *Side-facing seating position* |
| *Outboard seating positions* | | | *Centre seating position* | | |
| *Front* | *Other than front* | | *Front* | | *Other than front* |
| …. |  |  | |  | |  |  | | - |
| N1 | … | … | | … | | … | … | | - |
|  | … | | … | |  |  | | - |
| N2 | Br3, Br4m, Br4Nm orAr4m, Ar4Nm\* | B, Br3, Br4m, Br4Nm | | B, Br3, Br4m, Br4Nm, or A, Ar4m, Ar4Nm\* | | B, Br3, Br4m, Br4Nm | B, Br3, Br4m, Br4Nm | | - |
| N3 | Para. 8.1.6. lap belt permitted if the windscreen is outside the reference zone and for the driver's seat |  | | Para. 8.1.6. lap belt permitted if the windscreen is not in the reference zone | |  |  | | - |
| … | | | … | | … | | | … | |

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)