|  |  |
| --- | --- |
|  | E/ECE/324/Rev.1/Add.33/Rev.2/Amend.3−E/ECE/TRANS/505/Rev.1/Add.33/Rev.2/Amend.3 |
|  |  | 28 October 2016 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 33 – Regulation No. 34

 Revision 2 - Amendment 3

Supplement 1 to the 03 series of amendments – Date of entry into force: 8 October 2016

 Uniform provisions concerning the approval of vehicles with regard to the prevention of fire risks

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2016/8.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Annex 4,*

*Paragraph 2.5.4.,* amend to read:

"2.5.4. At the moment of collision the velocity of the centre of percussion of the pendulum shall be between 48 and 52 km/h."

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)