|  |  |
| --- | --- |
|  | E/ECE/324/Rev.2/Add.106/Rev.5/Amend.4−E/ECE/TRANS/505/Rev.2/Add.106/Rev.5/Amend.4 |
|  |  | 28 October 2016 |

 Agreement

 Concerning the Adoption of Uniform Technical Prescriptions for Wheeled Vehicles, Equipment and Parts which can be Fitted and/or be Used on Wheeled Vehicles and the Conditions for Reciprocal Recognition of Approvals Granted on the Basis of these Prescriptions[[1]](#footnote-2)\*

(Revision 2, including the amendments which entered into force on 16 October 1995)

\_\_\_\_\_\_\_\_\_

 Addendum 106 – Regulation No. 107

 Revision 5 - Amendment 4

Supplement 5 to the 05 series of amendments – Date of entry into force: 8 October 2016

 Uniform provisions concerning the approval of category M2 or M3 vehicles with regard to their general construction

This document is meant purely as documentation tool. The authentic and legal binding text is: ECE/TRANS/WP.29/2016/10.

**\_\_\_\_\_\_\_\_\_**

**UNITED NATIONS**

*Annex 3,*

*Paragraph 7.7.1.8.4.,* amend to read:

"7.7.1.8.4. When the seat is in the position of use, and when it is in the folded position, no part of it shall be:

 (a) Forward of a vertical plane passing through the centre of the seating surface of the driver's seat in its rearmost and lowest position and through the centre of the exterior rear-view mirror mounted on the opposite side of the vehicle or through the centre of any monitor used as device for indirect vision, whatever applicable,

 and

 (b) Above a horizontal plane which is located 300 mm above the centre of the seating surface of the driver's seat in its rearmost and lowest position."

*Annex 8,*

*Paragraph 3.10.1.,* correct to read:

"3.10.1. (Reserved)"

1. \* Former title of the Agreement: Agreement Concerning the Adoption of Uniform Conditions of Approval and Reciprocal Recognition of Approval for Motor Vehicle Equipment and Parts, done at Geneva on 20 March 1958. [↑](#footnote-ref-2)