|  |  |
| --- | --- |
|  | **INF.10** |
| **Economic Commission for Europe**Inland Transport Committee**Working Party on the Transport of Dangerous Goods****Joint Meeting of Experts on the Regulations annexed to theEuropean Agreement concerning the International Carriageof Dangerous Goods by Inland Waterways (ADN)(ADN Safety Committee)****Twenty-ninth session**Geneva, 22 - 25 August 2016Item 4(b) of the provisional agenda**Proposals for amendments to the Regulations annexed to ADN:****Other proposals** | English14 July 2016 |

 Proposal for amendment to Table C

 Transmitted by CEFIC (European Chemical Industry Council)

 I. Introduction

1. This proposal is submitted by CEFIC. The Safety Committee is invited to consider the amendment proposed below.

 II. Justification

2. Based upon the European Regulation on Classification, Labelling and Packaging of chemical substances and mixtures (CLP), the current classification in ADN needs to be amended. According to COMMISSION REGULATION (EU) No 286/2011 Toluene has to be classified for aquatic toxicity as chronic category 3, and this requires assignment to group “N2”. Therefore it is required to use a tank vessel type N23 instead of type N22.

 III. Proposal for amendment

3. The following amendments should be made to Table C:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| UN Nr | Name and description | Class | ClassificationCode | PG | Dangers | Type of tank vessel | Cargo tank design | Cargo tank type |
| (1) | (2) | (3a) | (3b) | (4) | (5) | (6) | (7) | (8) |
| 1294 | Toluene | 3 | F1 | II | Change “3 +N3” into “3 + N2” | N | 2 | Change “2” into “3” |