Proposal for amendments to the 01 series of amendments to Regulation No. 67 (Equipment for Liquefied Petroleum Gas)

The text reproduced below was prepared by the expert from the European Liquefied Petroleum Gas Association (AEGPL) to introduce tolerances for the dimensions of some filling units. The modifications to the current text of the Regulation are in bold for new characters.

**I. Proposal**

*Annex 9, paragraph 5,* amend to read:

“5. General design rules:

Paragraph 6.15.2., Provisions regarding the electrical insulation.

Paragraph 6.15.10., Provisions regarding the filling unit.

**For all dimensions of Figures 1, 2 and 4 without indication of tolerances, tolerances of class “medium” of EN 22768-1 shall apply.”**

II. Justification

Figure 1, 2 and 4 of annex 9, containing the drawings of dish, bayonet and acme filling units, do not contain tolerances for the dimensions required.

This lack of harmonization may create some problems in the connection of such filling units with the related nozzles with consequent potential safety risks