UNITED

NATIONS

Distr.

Economic and Social	GENERAL

Council	TRANS/WP.29/724
3 May 2000

ENGLISH

Original: ENGLISH and

FRENCH

ECONOMIC COMMISSION FOR EUROPE

INLAND TRANSPORT COMMITTEE

World Forum for Harmonization of Vehicle Regulations (WP.29)

DRAFT SUPPLEMENT 3	TO REGULATION No. 50

(Position, stop, direction indicator lamps for motorcycles)

Note: The text reproduced below was adopted by the Administrative Committee (AC.1) of the amended 1958 Agreement at its fourteenth session, following the recommendation by WP.29 at its one-hundred-and-twentieth session. It is based on document TRANS/WP.29/2000/13, not amended (TRANS/WP.29/703, para. 168).

__________

Paragraph 9., amend to read (footnote 5/ not modified):

" .....

The colour of the light emitted inside the field of the light distribution grid defined at paragraph 2 of annex 4, measured using a light source having a colour temperature of 2856 K, 5/ shall be within the limits of the co-ordinates prescribed for the colour in question in annex 5 to this Regulation. Outside this field no sharp variation of colour shall be observed.

However, for lamps equipped ....."

__________

GE.00-