|  |  |
| --- | --- |
| Note by the Secretariat | Informal document **GRRF-84-35**84th GRRF, 19-22 September 2017 Agenda item 7(i)  |

**Adopted amendment to tECE/TRANS/WP.29/GRRF/2017/21**

*Paragraph 2.3.,* amend to read:

"2.3. "*Tyre size designation*" means the designation as defined in paragraph 2.of Regulation No. 30 for class C1 tyres and paragraph 2**.** of Regulation No. 54 for class C2 and C3 tyres."

*Paragraph 2.9.,* amend to read:

"2.9. "*Run flat tyre*" means a tyre as defined in paragraph 2. of Regulation No. 30."

*Paragraph 2.18.,* amend to read:

"2.18. "*Speed category symbol*" means the symbol as defined in paragraph 2. of Regulation No. 30 for class C1 tyres and paragraph 2. of Regulation No. 54 for class C2."

*Paragraph 2.19.,* amend to read:

"2.19. "*Load capacity index*" means a number associated to the maximum load rating of the tyre in relation to the definition in paragraph 2. of Regulation No. 30 for class C1 tyres and paragraph 2. of Regulation No. 54 for class C2 tyres."

*Paragraph 5.2.2.2.1.,* amend to read:

"5.2.2.2.1. In the case of tyres of class C1, the "maximum load rating" as referred to in paragraph 2. of Regulation No. 30 is taken into account."

*Paragraph 5.2.2.2.2.,* amend to read:

"5.2.2.2.2. In the case of tyres of class C2, the "table load-capacity variation with speed" as referred to in paragraph 2. of Regulation No. 54 is taken into account, which shows, as a function of the load-capacity indices and nominal-speed-category symbols, the load variations which a pneumatic tyre can withstand taking into account the maximum design speed of the vehicle."

*Paragraph 5.2.3.1.2.,* amend to read:

"5.2.3.1.2. In the case of tyre of class C2, the speed category symbol shall be compatible with the maximum vehicle design speed and the applicable load/speed combination derived from the "Table load-capacity variation with speed" as described in paragraph 2. of Regulation No. 54."