|  |  |  |
| --- | --- | --- |
|  |  | **INF.12**  |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods 18 April 2018**

**104th session**

Geneva, 15-17 May 2018

Item 4 of the provisional agenda

**Work of the RID/ADR/ADN Joint Meeting**

Correction of the French version of P801

Transmitted by the Government of France

1. The Working Party adopted the following modification to packing instruction P801, additional requirement 2 in Chapter 4.1 (see page 25 of document ECE/TRANS/WP.15/240):

Replace “non-conductive” by “electrically non-conductive”.

2. The same amendment reads in French:

Ajouter « électrique » après « isolant ».

3. This amendment cannot be applied to additional requirement 2 in P801 worded in French as follows:

« Les accumulateurs empilés doivent être assujettis de manière adéquate sur plusieurs niveaux séparés par une couche en matériau non conducteur. »

4. We propose to replace the amendment to packing instruction P801, additional requirement 2 by the following:

4.1.4.1, instruction d’emballage P801 Dans la disposition supplémentaire 2, remplacer « non conducteur » par « non conducteur d’électricité ».

5. RID should be amended in the same way.