|  |  |
| --- | --- |
| Submitted by the experts from ETRTO | Informal document **GRRF-86-23**86th GRRF, 12-16 February 2018 Agenda item 7(c)  |

Proposal for amendments to ECE/TRANS/WP.29/GRRF/2018/5 and ECE/TRANS/WP.29/GRRF/2018/11

 I. Proposal

*Paragraph 3.4.,* amend to read:

"3.4. The markings referred to in paragraph 3.1. and the approval mark prescribed in paragraph 5.4. of this Regulation shall be moulded on to or into the tyres. They shall be clearly legible and shall, except for the marking referred to in paragraph**s** 3.1.1.**, 3.1.2. and 3.1.~~12.~~13.** above, be located on at least one lower sidewall."

 II. Justification

 The text proposed in ECE/TRANS/WP.29/GRRF/2017/5 and reflected in the consolidated document ECE/TRANS/WP.29/GRRF/2017/11 does not refer correctly to the proper paragraphs after the renumbering introduced due to the introduction of new paragraphs (Supplement 21). By separating para. 3.1. into paras. 3.1.1. and 3.1.2., para. 3.1.12. has become para. 3.1.13.