|  |  |
| --- | --- |
| Transmitted by the expert from The International Automotive Lighting and Light Signalling Expert Group (GTB) | Informal document **GRE-72-09**  (72nd GRE, 20 - 22 October 2014,  agenda item 4 (i) (iv)) |

**Proposal for Supplement 17 to the original series of Regulation No. 38 (Rear fog lamps)**

**I.** **Proposal**

*Paragraph 1.3.,* amend to read:

"1.3. “Rear fog lamps of different types” means lamps which differ in such essential respects as:

(a) the trade name or mark;

(b) The characteristics of the optical system (levels of intensity, light distribution angles, category of light source, light source module, etc.);

**(c) the variable intensity control, if any**.

A change of the colour of the light source or the colour of any filter does not constitute a change of type."

II. Justification

To correct an error introduced by Supplement 16 of the original series by ECE/TRANS/WP29/2012/71 (ECE/TRANS/WP.29/GRE/2011/10)