|  |  |  |
| --- | --- | --- |
|  |  | **INF.25**  |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Ninety-ninth session 12 November 2015**

Geneva, 9-13 November 2015

Item 6(b) of the provisional agenda

**Proposals for amendments to annexes A and B of ADR:**

**miscellaneous proposals**

 Alternative to the proposals in ECE/TRANS/WP.15/2015/8

 Transmitted by the Government of Switzerland

1.6.3.44

Fixed tanks (tank-vehicles) and demountable tanks intended for the carriage of UN Nos. 1202, 1203, 1223, 3475 and aviation fuel classified under UN Nos. 1268 or 1863, equipped with additive devices designed and constructed before 1 July 2015 in accordance with national provisions, but which do not, however, conform to the construction, approval and testing requirements of special provision 664 of Chapter 3.3 applicable as from 1 January 2015, may continue to be used until their first intermediate or periodic inspection after 31 December 2015. After this date, they shall only be used with the agreement of the competent authorities in the countries of use. **The following should be added to section 11. of the certificate of approval in 9.1.3.5 of fixed tanks (tank-vehicles) registered after 31. December 2016 : “Tank-vehicle with additive device in accordance with transitional measure 1.6.3.44.”.**

SP664 (e)  Transport document

Only the information required in accordance with 5.4.1.1.1 (a) to (d) needs to be added to the transport document for the additive concerned. **In that case for demountable tanks carried according to 1.6.3.44 the following shall also be entered in the transport document: " Demountable tank with additive device in accordance with transitional measure 1.6.3.44.**".