|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRSG/2015/35 | |
|  | **Economic and Social Council** | | Distr.: General  13 July 2015  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on General Safety Provisions**

**109th session**

Geneva, 29 September – 2 October 2015

Item 9 of the provisional agenda

**Regulation No. 67 (Equipment for Liquefied Petroleum Gas (LPG))**

Proposal for amendments to the 01 series of amendments to Regulation No. 67 (Equipment for Liquefied Petroleum Gas)

Submitted by the expert from the European Liquefied Petroleum Gas Association[[1]](#footnote-2)\*

The text reproduced below was prepared by the expert from the European Liquefied Petroleum Gas Association (AEGPL) to insert new safety provisions into UN Regulation No. 67 on Liquefied Petroleum Gas (LPG) systems having hydraulic interconnections with the petrol or diesel fuelling system through which inter-flows of fuels may occur. The modifications to the current text of Regulation No. 67 are marked in bold characters.

**I. Proposal**

*Insert new paragraphs 2.21. to 2.23.,* to read:

"**2.21. "LPG-system" means a set of LPG specific equipment intended to be fitted in a vehicle to constitute an integrated and functional whole aimed at enabling the propulsion with LPG;**

**2.22. "Interconnected LPG-system" means a LPG-system having interconnections with the petrol or diesel fuelling system that include a hydraulic path through which flows of petrol or diesel into the LPG container, or vice versa, may occur;**

**2.23. "Multi-component": means a device consisting of all or part of specific equipment mentioned in paragraph 2.2**."

*Paragraphs 6.4. to 6.14. (former),* amend to read (inserting a new paragraph 6.15.):

"6.4. - 6.**15**. Provisions regarding other components

The other components, which are shown in Table 1, shall be type approved pursuant to the provisions laid down in the annexes which can be determined from the table.

Table 1

| *Paragraph* | *Component* | *Annex* |
| --- | --- | --- |
| 6.4. | Fuel pump | 4 |
| 6.5. | Vaporizer1  Pressure regulator1 | 6 |
| 6.6. | Shut-off valves  Non-return valves  Gas-tube pressure relief valves  Service couplings | 7 |
| 6.7. | Flexible hoses | 8 |
| 6.8. | Filling unit | 9 |
| 6.9. | Gas injection devices/Gas mixing piece3  or  Injectors | 11 |
| 6.10. | Gas dosage units2 | 12 |
| 6.11. | Pressure sensors  Temperature sensors | 13 |
| 6.12. | Electronic control unit | 14 |
| 6.13. | LPG filter units | 5 |
| 6.14. | Pressure relief device | 3 |
| **6.15.** | **Multi-component** | **Annexes applicable to the single components** |

1 Either combined or separate

2 Only applicable when the gas dosage actuator is not integrated in the gas injection device.

3 Applicable only when the operating pressure of the gas mixing piece exceeds 20 kPa (Class 2)."

*Paragraphs 6.15. to 6.15.1.5. (former),* renumber as paragraphs 6.16. to 6.16.1.5.

*Insert a new paragraph 6.16.1.6.,* to read:

"**6.16.1.6. When the 80 per cent stop valve is intended to be fitted as a component of an interconnected LPG-system, the manufacturer shall demonstrate to the type approval authority that the safety concept of the LPG-system prevents an overfilling of the container**."

*Paragraphs 6.15.2. to 6.15.13.2.4. (former),* renumber as paragraphs 6.16.2. to 6.16.13.2.4.

*Insert a new paragraph 6.17.,* to read:

"**6.17. When intended to be fitted as components or parts of an interconnected LPG-system, non-metallic, metallic or a mixture of metallic and non-metallic LPG components, including flexible hoses and their elements, and non-metallic, metallic or a mixture of metallic and non-metallic parts of LPG components which may come into contact with petrol shall meet the requirements specified in Annex 18 to this Regulation.**

**Non-metallic, metallic or a mixture of metallic and non-metallic components or components containing non-metallic parts shall bear an approval mark according to Annex A, appendix 1.**"

*Insert new paragraphs 17.13. to 17.13.2.4.,* to read:

"**17.13. Specific provisions for interconnected LPG-systems**

**17.13.1. LPG-system for dual-fuel (LPG-diesel) vehicle**

**17.13.1.1. The manufacturer shall demonstrate to the technical service that the safety concept of the LPG-system prevents any flow of LPG into the diesel tank.**

**If the technical service deems that the safety concept is not fully effective in preventing such flows, the technical service may require to implement appropriate provisions to remove from the diesel tank any amount of LPG that is likely to flow, as soon as the vehicle is run in diesel mode.**

**17.13.1.2. The manufacturer shall demonstrate to the technical service that the safety concept of the LPG-system prevents any flow of diesel into the LPG container.**

**If the technical service deems that the safety concept is not fully effective in preventing such flows, the technical service may require to implement appropriate provisions to remove from the LPG container any amount of diesel that is likely to flow, as soon as the vehicle is run in dual fuel mode.**

**17.13.2. LPG-system for bi-fuel (LPG-petrol) vehicle**

**17.13.2.1. The manufacturer shall demonstrate to the technical service that the safety concept of the LPG-system prevents any flow of LPG into the petrol tank.**

**If the technical service deems that the safety concept is not fully effective in preventing such flows, the technical service may require to implement appropriate provisions to remove from the petrol tank any amount of LPG that is likely to flow, as soon as the vehicle is run in petrol mode.**

**17.13.2.2. In order to prevent that flows of petrol into LPG container, occurring during switch-over operations, could lead to an overfilling of the LPG tank (i.e. above 80 per cent of its capacity which means 80 per cent liquid and 20 per cent gaseous fuel), the LPG-system shall contain an Electronic Control Unit complying also with paragraph 6. of Annex 14.**

**The manufacturer shall demonstrate to the technical service that the safety concept of the LPG-system prevents any flow of petrol into the LPG container during operations other than switch-over ones.**

**If the technical service deems that the safety concept is not fully effective in preventing such flows, the technical service may require to implement appropriate provisions to remove from the LPG container any amount of petrol that is likely to flow, as soon as the vehicle is run in LPG mode.**

**17.13.2.3. Means shall be provided to prevent that flows of petrol into the LPG fuel container could lead to a content of petrol higher than 16 per cent of the actual volume contained in the LPG tank.**

**This measure shall be demonstrated in accordance with the procedures laid down in Annex 19.**

**The present requirement shall be fulfilled also in case of faults, e.g. by use of redundant components, activation of limp home mode or of a malfunction indication to the driver.**

**17.13.2.4. Non-metallic, metallic or a mixture of metallic and non-metallic LPG components, including flexible hoses and their elements, and non-metallic, metallic or a mixture of metallic and non-metallic parts of LPG components which may come into contact with petrol shall comply with the requirements set out in paragraph 6.17**."

*Annex 1, add new items 1.2.6. and 1.2.7.,* to read:

"**1.2.6. Documentation of the safety concept and system description/drawings to avoid overfilling of the LPG tank (paragraph 17.3.2.2.):**

**1.2.7. Documentation of the safety concept for interconnected LPG systems (Annex 19):** "

*Annex 2A, insert new Appendix 1,* to read:

**"Annex 2A - Appendix 1**

**Arrangement of the type-approval mark of non-metallic, metallic or a mixture of metallic and non-metallic LPG components and LPG components containing non-metallic, metallic or a mixture of metallic and non-metallic parts compatible with petrol. The letter N indicates non-metallic components. The letter M indicates metallic components. The letters NM indicates a combination of metallic and non-metallic components. (See paragraph 6.17. of this Regulation)**



**67 R—012439-NM CLASS #1**

**a ≥ 5 mm**

**1 Class 0, 1, 2, 2A or 3**

**The above approval mark shall be affixed to the LPG component or to an identification plate to be placed in the engine compartment on a visible fixed irreplaceable chassis part, when the component is to be installed in such a way that will no longer be readily accessible.**

**The approval mark shows that the component has been approved in the Netherlands (E4), pursuant to Regulation No. 67 under approval number 012439. The first two digits of the approval number indicate that the approval was granted in accordance with the requirements of Regulation No. 67 as amended by the 01 series of amendments**."

*Annex 14, insert new paragraphs 6. to 6.2.,* to read:

"**6. When the electronic control unit (ECU) is intended to be fitted as a component of an interconnected LPG-system, it shall inhibit, by controlling the fuel selection system, the vehicle operation in petrol mode after each switch-over operation to LPG mode until a volume of liquid fuel equivalent to that flown into the LPG tank during such an operation is consumed.**

**Notwithstanding this, the ECU may permit the switch over to petrol mode if a fault in the LPG-system determines the inoperability of the system. Such a fault shall be clearly indicated to the driver.**

**In case of the inoperability of the LPG-system, the safety concept of the LPG-system shall prevent any flow of petrol into the LPG container after switching-over to petrol mode.**

**The ECU shall bear a marking with the following data clearly legible and indelible:**

**(a) the wording "ICS", and**

**(b) the approval mark according to paragraph 5.4. of this Regulation.**

**6.1. In order to measure the volume of liquid fuel that flows during the switch-over operations, the following test shall be carried out:**

**(a) Install the LPG-system other than the container on a vehicle;**

**(b) Place the container on a weighing system and fill up the LPG tank;**

**(c) After having pressurized the LPG-system up to the normal operating conditions, record the reading of the weighing system (W1);**

**(d) Disable the ECU feature described in paragraph 6. above;**

**(e) Switch-over from LPG to petrol and vice versa for at least 10 times;**

**(f) Record the reading of the weighing system (W2);**

**The volume of petrol flown per switch-over operation shall be calculated as follows:**

**Vsw = (W2-W1) / #SW / Dpetrol**

**where:**

**Dpetrol = 743 kg/m3;**

**#SW = number of switch-over operations from LPG to petrol mode and vice versa during the test.**

**The weighing system shall have the following:**

**(a) A precision of ± 0.02 per cent of full scale or better;**

**(b) A resolution of 20 g;**

**(c) An accuracy of ± 2 per cent of the reading or ± 0.3 per cent of full scale whichever is better.**

**6.2. In order to verify compliance with paragraph 6. of this annex, the ECU shall be tested as follows:**

**(a) Install the LPG-system on a vehicle;**

**(b) Set the fuel selection system in LPG mode;**

**(c) Warm up the engine until all temperatures of cooling and lubrication means and the pressure of lubrication means have reached equilibrium.**

**(d) Let the engine run at the lowest idling speed;**

**(e) Switch over from LPG mode to petrol mode and vice versa;**

**(f) Set the fuel selection system in petrol mode.**

**Test interpretation**

**The criteria adopted for the interpretation of the test is as follows:**

**(i) Petrol mode is disabled until a volume of liquid fuel equal to Vsw, as calculated in paragraph 6.1. above, is consumed. Such consumption may be calculated making use of the fuel flow signals of the LPG ECU read out by means of an appropriate scan tool.**

**The test shall be repeated also at the highest idling speed**."

*Insert a new Annex 18,* to read:

**"Annex 18**

**Provisions regarding compatibility of metallic and non-metallic components and parts with petrol**

**1. Requirements for metallic and non-metallic components and parts**

**1.1. Non-metallic components or parts which may come into contact with petrol shall not show excessive volume change or loss of weight.**

**Resistance to petrol according to ISO 1817 with the following conditions:**

**(a) Medium: petrol (E10) complying with Annex 10 to Regulation No. 83;**

**(b) Temperature: 23 °C (tolerance according to ISO 1817);**

**(c) Immersion period: 72 hours.**

**1.1.1. Requirements for non-metallic components and parts:**

**Maximum change in volume 20 per cent;**

**After storage in air with a temperature of 40 ºC for a period of 48 hours, the mass compared to the original value may not decrease more than 5 per cent.**

**1.3. Metallic components or parts which may come into contact with petrol shall have a permanent resistance against petrol. Metallic parts shall permanently be protected against corrosion (e.g. coating, surface finish, material mix) and fulfil the requirements of Annex 15, paragraph 12**."

*Insert a new Annex 19,* to read:

**"Annex 19**

**Provisions regarding interconnected LPG-systems**

**1. Documentation**

**1.1. The following documentation shall be provided to the Type-Approval Authority and to the Technical Service:**

**(a) The description of the safety concept used to ensure compliance with the requirements specified in paragraph 17.13.2.3. of this Regulation, including all equipment, monitored parameters, relevant factors, criteria and actions;**

**(b) A detailed flowchart that depicts the strategies used for the purposes of meeting the requirements specified in paragraph 17.13.2.3.** **of this Regulation**

**2. Test procedures**

**2.1. In order to verify compliance with paragraph 17.13.2.3.** **of this Regulation, a vehicle shall be tested as follows:**

**Test procedure**

**(a) Install the LPG equipment on the vehicle;**

**(b) Fill up the LPG tank with at least 10 liters of fuel;**

**(c) Set the fuel selection system in LPG mode;**

**(d) Let the engine run at the lowest idling speed;**

**(e) Switch over from LPG mode to petrol mode and vice versa;**

**(f) Repeat the action (e) until the disablement of petrol mode becomes permanent;**

**Test interpretation**

**The criteria adopted for the interpretation of the test is as follows:**

**Nsw < 0.16 \* Vin / Vsw**

**where:**

**Nsw = the number of switch-over operations from LPG mode to petrol mode and vice versa until the disablement of petrol mode becomes permanent.**

**Vsw = the volume of petrol flown into the LPG tank per switch-over operation as measured in paragraph 6.1. above**."

II. Justification

A. Introduction

A.1. The proposed amendments aim, overall, at improving the safety aspects of gas systems which, by their architectural nature, allow limited flows of petrol into the LPG tank. This is, for instance, the case of the current LPG direct injection systems, in all the versions available today on the market, regardless of the manufacturer: in the rare cases in which the system acts, automatically or upon user's request, a switch over between operational modes (for example, when the LPG tank is nearing empty) a small flow of petrol is flushed into the LPG tank.

A.2. The unconditioned prohibition of such reverse flows would determine the unjustifiable ban from the market of such innovative systems to the detriment of the environment, as these new gas systems significantly reduce the emission of pollutants and greenhouse gases with respect to analogous petrol technologies.

A.3. In general, it is observed that:

(a) the presence of petrol in the LPG tank does not create pressure-related risks as it has a lower volatility, indeed its mixing with the gaseous fuel can only reduce the internal pressure at the same temperatures,

(b) the flush of petrol into the LPG tank is triggered only by the switch-over from an operational mode to the other one, and since the gas fuelling system cranks, warms up and runs only on gas, this event is very rare, especially if compared to the other technologies where petrol is used also in gas mode during the driving cycle,

(c) petrol has got a vapour pressure and a thermal expansion coefficient that are negligible, hence, the presence of some amount of petrol (very small) in place of LPG improves the safety level as regards the pressure-related risks,

(d) 80 per cent is a rather conservative filling limit, with a significant margin versus 85 per cent, that is the correct one, as established also in TPED and PED directives,

(e) overfilling of the LPG tank will be prevented by the strategy proposed in this document: each single flushed volume shall be removed by disabling the switch-over from LPG to petrol until this volume is fully consumed; relevant sound laboratory tests have been proposed.

B. Detailed justifications

B.1. New paragraph 2.20. introduces the definition of a generic "LPG-system". Although "LPG-system" is referred to in the current Regulation in several points, this lacks a proper definition.

B.2. New paragraph 2.21., in defining a particular LPG-system, the "Interconnected LPG-system", clarifies the scope of the provisions that are proposed in this amendment.

It is worth noting that this new specific definition excludes LPG-systems with no hydraulic interconnections with the petrol/diesel fuelling system as well as systems with interconnections that do not include a hydraulic path through which flows of petrol or diesel into the LPG tank may occur.

As for "petrol or diesel fuelling system", it is implicitly meant the hydraulic circuit upstream the fuel injection/aspiration point.

B.3. With new paragraph 2.22., a proper definition of "multi-component" is introduced, filling an evident gap in the Regulation: several points refers to it without a specific definition.

New paragraph 6.15. aims at clarifying the requirements and tests of the Regulation that are applicable to a "multi-component"

Both paragraphs 2.22. and 6.15. are of particular relevance to this amendment proposal because one of the main components of the LPG DI system is a multi-component, that is usually commercialized with the name of FSU (Fuel Selection Unit).

B.4. New paragraph 6.16.1.6. requires that, during the approval procedure of a 80 percent stop intended to be fitted in an interconnected LPG-system, the safety concept of the whole system aimed to prevent the LPG container overfilling shall be demonstrated.

B.5. New paragraph 6.17. requires an appropriate compatibility test with petrol to the LPG components or parts of interconnected LPG-systems that may come into contact with petrol. A distinctive marking for such components or components containing such parts is also required.

B.6. New paragraph 17.13. includes the requirements for the interconnected LPG-systems, opening a distinction between dual-fuel (LPG-diesel) vehicle (paragraph 17.13.1.) and bi-fuel (LPG-petrol) vehicle (paragraph 17.13.2.).

**In a dual-fuel vehicle**, both flows of LPG fuel into the diesel tank and vice versa are prevented by requiring the implementation of an appropriate safety, respectively in paragraphs 17.13.1.1. and 17.13.1.2.

A safeguard clause has been added to ensure that proper means are provided to remove any amount of LPG into the diesel tank (or vice versa) if the technical service deems not fully effective the safety concept implemented by the manufacturer.

**In a bi-fuel vehicle,** flows of LPG fuel into the petrol tank are prevented by requiring the implementation of an appropriate safety concept (paragraph 17.13.2.1., first sentence).

In the case, the safety concept is deemed not fully effective by the technical service, proper means are required to remove any amount of LPG from the petrol tank as soon as the vehicle runs on petrol mode (paragraph 17.13.2.1., second sentence).

Flows of petrol into the LPG tank are permitted only during switch-over operations and under certain conditions aimed at preventing the LPG tank overfilling (paragraph 17.13.2.2.) and the petrol over-blending into LPG (paragraph 17.13.2.3.), above the limit set out in Regulations Nos. 83 and 115 (20 per cent by energy).

During operations other than switch-over ones, flows of petrol shall be prevented by the implementation of an appropriate safety concept.

The manufacturer shall demonstrate to the technical service that the safety concept is fully effective in preventing such flows; if not, proper means are required to remove any amount of petrol from the LPG container as soon as the vehicle runs in gas mode.

B.7. In order to prevent the overfilling of the LPG container due to possible flows of petrol, occurring during the switch-over operations, the ECU of an interconnected LPG-system shall comply with the new paragraph 6. of Annex 14, in addition to the other applicable requirements (paragraph 17.1.2.2.).

Paragraph 6. of Annex 14 requires the ECU to be capable to consume an equivalent volume of each single petrol flush when this occurs due to a switch-over operation.

In other words, ECU shall inhibit the switch back to petrol until such a volume is consumed.

A derogation from such a temporary disablement of petrol mode is possible only in the case the LPG-system becomes inoperable as consequence of an internal fault, to avoid putting the vehicle in a more hazardous condition.

Two tests methods are proposed to measure the average petrol flush volume as well as to prove the capability of the ECU to inhibit the switch back to petrol after a flush occurs, respectively in paragraphs 6.1. and 6.2. of Annex 14.

B.8. In order to prevent the over-blending of petrol into the LPG, the interconnected LPG system as a whole shall fulfil the provisions set out in new Annex 19 (paragraph 17.13.2.3).

Annex 19, paragraph 1.1., requires providing the type-approval authority and the technical service with a proper documentation describing the equipment and the strategy used to prevent the over-blending.

The LPG-system shall be capable to set the permanent disablement of petrol mode (i.e. disablement until LPG container gets empty) when the concentration of petrol into the actual liquid fuel in the LPG tank exceeds the max blending limit of 16 per cent by volume (equivalent to 20 per cent in energy as required by Regulations Nos. 83 and 115).

A performance test is required to demonstrate the compliance of such a max blending limit (16 per cent by volume), comparing the number of switch-over operations before the petrol mode disablement becomes permanent with the number that would cause (by a conservative calculation) the over-blending.

The proposed formula is justified by the following:

(a) The concentration of petrol into LPG just after the first switch-over will be Vsw/(Vin +Vsw); where Vsw is the volume flushed when switching over and Vin is the initial volume of LPG;

(b) At each further switch-over an additional concentration, equal to Vsw/Vin, will be added, considering that the same volume (Vsw) of liquid fuel will be (first) consumed and (then) injected;

(c) Since Vsw can be considered negligible in comparison with Vin, the concentration at i switch-over operation will be Ci=i\*Vsw/Vin. Therefore, i‑max shall be less than 0.16\*Vin/Vsw.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2012–2016 (ECE/TRANS/224, para. 94 and ECE/TRANS/2012/12, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)