Economic Commission for Europe

Inland Transport Committee

Working Party on the Transport of Dangerous Goods

**Joint Meeting of Experts on the Regulations annexed to the**

**European Agreement concerning the International Carriage**

**of Dangerous Goods by Inland Waterways (ADN)**

**(ADN Safety Committee)**

**Twenty-eighth session**

Geneva, 25-29 January 2016

Item 5 (b) of the provisional agenda

**Proposals for amendments to the Regulations annexed to ADN:
Other proposals**

 Proposal for additions to Table C

 Transmitted by the Central Commission for the Navigation of the Rhine (CCNR)[[1]](#footnote-1)

1. It has been found that, for the following entries in table C,

UN No. 1986 ALCOHOLS, FLAMMABLE, TOXIC, N.O.S.,

UN No. 1992 FLAMMABLE LIQUID, TOXIC, N.O.S,

UN No. 2924 FLAMMABLE LIQUID, CORROSIVE, N.O.S. and

UN No. 3286 FLAMMABLE LIQUID, TOXIC, CORROSIVE, N.O.S.

the rows on transport in pressure tanks are missing for packing group I.

2. The informal working group on substances considered this matter at its seventh and eighth meetings and recommended adding the relevant rows to Table C (informal document INF.12 from the twenty-seventh session).

3. It is proposed that the following four rows should be added to table C:

| *(1)* | *(2)* | *(3a)* | *(3b)* | *(4)* | *(5)* | *(6)* | *(7)* | *(8)* | *(9)* | *(10)* | *(11)* | *(12)* | *(13)* | *(14)* | *(15)* | *(16)* | *(17)* | *(18)* | *(19)* | *(20)* |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *UN No. or substance identification No.* | *Name and description* | *Class* | *Classification code* | *Packing group* | *Dangers* | *Type of tank vessel* | *Cargo tank design* | *Cargo tank type* | *Cargo tank equipment* | *Opening pressure of the high-velocityvent valve in kPa* | *Maximum degree of filling in %* | *Relative density at 20 °C* | *Type of sampling device* | *Pump room below deck permitted* | *Temperature class* | *Explosion group* | *Anti-explosion protection required* | *Equipment required* | *Number of cones/blue lights* | *Additional requirements/remarks* |
|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| 1986 | ALCOHOLS, FLAMMABLE, TOXIC, N.O.S.  | 3 | FT1 | I | 3+6.1+(N1, N2, N3, CMR, F or S) | C | 1 | 1 | \* | \* | 95 |   | 1 | no | T4 3) | II B4) | yes | PP, EP, EX, TOX, A | 2 | 27; 29; \*see 3.2.3.3 |
| 1992 | FLAMMABLE LIQUID, TOXIC, N.O.S. | 3 | FT1 | I | 3+6.1+(N1, N2, N3, CMR, F or S) | C | 1 | 1 | \* | \* | 95 |   | 1 | no | T4 3) | II B4) | yes | PP, EP, EX, TOX, A | 2 | 27; 29\*see 3.2.3.3 |
| 2924 | FLAMMABLE LIQUID, CORROSIVE, N.O.S. | 3 | FC | I | 3+8+(N1, N2, N3, CMR,F or S) | C | 1 | 1 | \* | \* | 95 |   | 1 | yes | T4 3) | II B4) | yes | \* | 1 | 27; 29\*see 3.2.3.3 |
| 3286 | FLAMMABLE LIQUID, TOXIC, CORROSIVE, N.O.S. | 3 | FTC | I | 3+6.1+8+(N1, N2, N3, CMR, F or S) | C | 1 | 1 | \* | \* | 95 |   | 1 | no | T4 3) | II B4) | yes | PP, EP, EX, TOX, A | 2 | 27; 29\*see 3.2.3.3 |

1. Distributed in German by the Central Commission for the Navigation of the Rhine in document CCNR-ZKR/ADN/WP.15/AC.2/2016/6. [↑](#footnote-ref-1)