|  |  |
| --- | --- |
| Submitted by the Working Party on Brakes and Running Gear (GRRF) | Informal document **WP.29-170-06**(170th WP.29, 15-18 November 2016,agenda item 4.13.1) |

Proposal to amend the proposal for the 04 series of amendments to Regulation No. 78 (Motorcycle Braking) (ECE/TRANS/WP.29/2016/114)

I. Proposal

*In ECE/TRANS/WP.29/2016/114*,

*New paragraph 5.1.16, item (e) and (f),* amend to read:

"(e) The disablement of the antilock brake system function shall be indicated by the activation of symbol B.18 as specified in ISO 2575:2010 (ISO 7000-2623) or any other equivalent unequivocal indication of the disabled antilock brake system state. Alternatively the warning lamp referred to in paragraph 5.1.13. shall be continuously activated (i.e. lit or flashing); and

(f) Prohibition of any software and/or hardware defeat device compromising or allowing to circumnavigate one or more of the requirements set out in points (a) to (e)**;** and"

II. Justification

At its eighty-second session, GRRF reconfirmed the submission of the proposal for a new 04 series of amendments to Regulation No. 78, as amended above.

\_\_\_\_\_\_\_\_\_\_\_