|  |
| --- |
| **UN/SCETDG/51/INF.41** |
| **Committee of Experts on the Transport of Dangerous Goodsand on the Globally Harmonized System of Classificationand Labelling of Chemicals****Sub-Committee of Experts on the Transport of Dangerous Goods 5 July 2017****Fifty-first session**Geneva, 3-7 July 2017Item 6 (a) of the provisional agenda**Miscellaneous proposals for amendments to the Model Regulationson the Transport of Dangerous Goods: marking and labelling** |

 Specification of hazard labels and marks

 Submitted by the International Air Transport Association (IATA)

 Proposal

1. Based on the discussion of INF.17, the following is proposed to remove reference to the line on hazard labels being a minimum of 2 mm thick and also to provide some tolerance for the distance from the line forming the diamond on hazard labels being 5 mm to the edge of the label.

5.2.2.2.1.1.2 The label shall be in the form of a square set at an angle of 45 degrees (diamond-shaped). The minimum dimensions shall be 100 mm x 100 mm. There shall be a line inside the edge forming the diamond which shall be parallel and [approximately] 5 mm from the outside of that line to the edge of the label.