|  |  |  |
| --- | --- | --- |
|  | **INF.31** | |
| **Economic Commission for Europe**  Inland Transport Committee  **Working Party on the Transport of Dangerous Goods**  **Joint Meeting of Experts on the Regulations annexed to the European Agreement concerning the International Carriage of Dangerous Goods by Inland Waterways (ADN) (ADN Safety Committee)**  **Thirty-first session**  Geneva, 28-31 August 2017 Item 3 (c) of the provisional agenda  **Implementation of the European Agreement concerning the International Carriage of Dangerous Goods by Inland Waterways (ADN):**  **interpretation of the Regulations annexed to ADN** | | German  28 August 2017 |

Shower and eye/face bath, transitional provision

Transmitted by EBU, ERSTU and ESO

1. Der Sicherheitsausschuss hat bei seiner 31. Sitzung beschlossen, den Wortlaut von 9.3.x.60 zu verändern.

2. Die Vertreter des Binnenschifffahrtsgewerbes bitten um die Aufnahme folgender Übergangsregelung:

|  |  |  |
| --- | --- | --- |
| **Absatz** | **Inhalt** | **Frist und Nebenbestimmungen** |
| 9.3.x.60 | Das Wasser muss der Qualität des Trinkwassers an Bord entsprechen.  Es muss ein federbelastetes Rückschlagventil montiert sein. | N.E.U., Erneuerung des Zulassungszeugnisses nach dem 31.12.2023 |