|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRE/2017/23 | |
| _unlogo | **Economic and Social Council** | | Distr.: General  4 August 2017  Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Lighting and Light-Signalling**

**Seventy-eighth session**

Geneva, 24–27 October 2017

Item 6 (a) of the provisional agenda

**Regulation No. 48 (Installation of lighting and light-signalling devices) -**

**Proposals for amendments to the 05 and 06 series of amendments**

Proposal for Supplement 11 to the 06 series of amendments to Regulation No. 48 (Installation of lighting and light-signalling devices)

**Submitted by the experts from the Czech Republic and Italy, with the support of the Task Force on Headlamp Switching (TF HS)**[[1]](#footnote-2)\*

The text reproduced below was prepared by the experts from Czech Republic and Italy, with the support of TF HS, to correct and clarify the requirements for daytime running lamps (DRL) in conjunction with rear position lamps. The modifications to the existing text of the Regulation are marked in bold for new or strikethrough for deleted characters.

**I. Proposal**

*Add a new paragraph 5.11.1.3.*, to read:

“**5.11.1.3. When light signalling system operates according to paragraph 6.19.7.4.**”

*Paragraph 6.2.7.7.*, amend to read:

“6.2.7.7. Without prejudice to paragraph 6.2.7.6.~~1~~., the dipped-beam headlamps may switch ON and OFF automatically relative to other factors such as time or ambient conditions (e.g. time of the day, vehicle location, rain, fog, etc.).”

*Paragraph 6.9.8.*, amend to read:

“6.9.8 Tell-tale

Circuit-closed tell-tale mandatory. This tell-tale shall be non-flashing and shall not be required if the instrument panel lighting can only be switched ON simultaneously with the front position lamps.

**This requirement does not apply when light signalling system operates according to paragraph 6.19.7.4.**

However, a tell-tale indicating failure is mandatory if required by the component regulation.”

*Paragraph 6.10.8.*, amend to read:

“6.10.8 Tell-tale

Circuit-closed tell-tale mandatory. It shall be combined with that of the front position lamps.

**This requirement does not apply when light signalling system operates according to paragraph 6.19.7.4.**

However, a tell-tale indicating failure is mandatory if required by the component regulation.”

*Paragraph 6.19.7.4.*, amend to read:

“6.19.7.4. The lamps referred to in paragraph 5.11. may be switched ON when the daytime running lamps are switched ON. **If this option is chosen, at least the rear position lamps shall be switched ON.**”

II. Justification

1. At its seventy-seventh session, GRE adopted draft supplement [10] to the 06 series of amendments to Regulation No. 48, amending the provisions on automatic switching between DRLs and headlamps (ECE/TRANS/WP.29/GRE/77, para. 19 and Annex II to the report). The proposal removed several subparagraphs (including 5.11.1.3.) that had transitional application only for the 05 series of amendments, but were kept by mistake in the 06 series of amendments as well.

2. However, during its first two meetings, TF HS decided to retain the possibility to switch ON DRLs in conjunction with at least rear position lamps, without the need for the position lamps tell-tale in that case. This solution is necessary for some countries and is also logical from an energy saving perspective, because not all other lamps (referred to in paragraph 5.11.) necessarily need to be switched ON.

3. In addition, this proposal corrects a wrong reference to the deleted paragraph in paragraph 6.2.7.7., which was introduced by draft supplement [10] to the 06 series of amendments to Regulation No. 48.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2016–2017 (ECE/TRANS/254, para. 159 and ECE/TRANS/2016/28/Add.1, cluster 3.1), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)