|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.29/GRRF/2017/4 |
| Description: _unlogo | **Economic and Social Council** | Distr.: General10 November 2016Original: English |

**Economic Commission for Europe**

Inland Transport Committee

**World Forum for Harmonization of Vehicle Regulations**

**Working Party on Brakes and Running Gear**

**Eighty-third session**

Geneva, 23-27 January 2017

Item 7(c) of the provisional agenda

**Tyres: Regulation No. 54**

Proposal for amendments to Regulation No. 54 (Tyres for commercial vehicles and their trailers)

Submitted by the experts from the European Tyre and Rim Technical Organisation[[1]](#footnote-2)\*

The text reproduced below was prepared by the experts from the European Tyre and Rim Technical Organisation (ETRTO) in order to amend Annex 5 to Regulation No. 54. The modifications to the existing text of the Regulation are marked in bold for new or strikethrough for deleted characters.

1. Proposal

*Annex 5, part II, Table B,* add the following entries:

"

| *Tyre-sizedesignation (+)* | *Measuring rim width code* | *Nominal rim diameterd (mm)* | *Outer diameterD (mm)* | *Section widthS (mm)* |
| --- | --- | --- | --- | --- |
|  |  |  | *Normal* | *Snow* |  |
| **…****33x11.50R20LT****35x11.50R17LT****37x13.50R26LT****36x15.50R20LT****40x15.50R26LT****…** | **9.00****9.00****11.00****12.50****12.50** | **508****432****660****508****660** | **826****877****928****902****1004** | **832****883****934****908****1010** | **290****290****345****395****395** |

"

II. Justification

 It is proposed to add these sizes as they are to be sold in countries requiring Type Approval according to Regulation No. 54.

1. \* In accordance with the programme of work of the Inland Transport Committee for 2010–2014 (ECE/TRANS/208, para. 106 and ECE/TRANS/2010/8, programme activity 02.4), the World Forum will develop, harmonize and update Regulations in order to enhance the performance of vehicles. The present document is submitted in conformity with that mandate. [↑](#footnote-ref-2)