Proposal for draft amendments to UN Regulation No. 43 (Safety glazing)

The text reproduced below was prepared by the expert from OICA to remove some inconsistencies between UN GTR No. 6 and UN Regulation No. 43. This document comes in addition to ECE/TRANS/WP.29/GRSG/2017/15.The modifications to the current text of Regulation No. 43 are marked in bold characters for new and strikethrough for deleted characters.

**I. Proposal**

*Annex 21, paragraph 1.3.1.,* amend Table 2 to read:

"Table 2

| *Seat-back angle**(in °)* | *Horizontal co-ordinates**X* | *Vertical co-ordinates**Z* | *Seat-back angle**(in °)* | *Horizontalco-ordinates**X* | *Verticalco-ordinates**Z* |
| --- | --- | --- | --- | --- | --- |
| 5678910111213141516171819202122 | - 186 mm~~- 176~~ **-177** mm- 167 mm- 157 mm- 147 mm- 137 mm- 128 mm- 118 mm- 109 mm- 99 mm- 90 mm- 81 mm~~- 71~~ **-72**  mm- 62 mm- 53 mm- 44 mm- 35 mm- 26 mm | 28 mm27 mm27 mm~~26~~ **27** mm26 mm25 mm24 mm23 mm22 mm21 mm20 mm18 mm17 mm15 mm13 mm11 mm 9 mm 7 mm | 232425262728293031323334353637383940 | - 17 mm- 9 mm0 mm9 mm17 mm26 mm34 mm43 mm51 mm59 mm67 mm76 mm84 mm92 mm100 mm107 mm115 mm123 mm |  5 mm 2 mm 0 mm- 3 mm- 5 mm- 8 mm- 11 mm- 14 mm~~- 17~~ **-18** mm- 21 mm- 24 mm- 28 mm~~- 31~~ **-32** mm- 35 mm- 39 mm- 43 mm- 47 mm- 52 mm |

"

**II. Justification**

Alignment with the corresponding values in UN GTR No. 6 and UN Regulation No. 125. This document completes ECE/TRANS/WP.29/GRSG/2017/15 and does not supersede it.