|  |
| --- |
| **UN/SCETDG/53/INF.54** |
| **Committee of Experts on the Transport of Dangerous Goodsand on the Globally Harmonized System of Classificationand Labelling of Chemicals****Sub-Committee of Experts on the Transport of Dangerous Goods 21 June 2018****Fifty-third session**Geneva, 25 June-4 July 2018Item 6 (c) of the provisional agenda**Miscellaneous proposals for amendments to the Model Regulations on the Transport of Dangerous Goods:portable tanks** |

 Design pressure calculations

 Transmitted by the expert from the Russian Federation

 Introduction

1. Paragraph 6.7.3.1 of the UN Recommendations on the Transport of Dangerous Goods, Model Regulations says:

*“Design pressure means the pressure to be used in calculations required by a recognized pressure vessel code. The design pressure shall be not less than the highest of the following pressures:*

*(a) The maximum effective gauge pressure allowed in the shell during filling or discharge, or*

*(b) The sum of:*

*(i) the maximum effective gauge pressure to which the shell is designed as defined in (b) of the MAWP definition,*

*(ii) a head pressure determined on the basis of the static forces specified in 6.7.3.2.9 but not less than 0.35 bar.”.*

2. The expert from the Russian Federation understands this to be applicable for the stand-alone vessel design pressure calculation, not for portable tanks.

3. The design pressure calculation for the portable tank seems not to comply with 6.7.3.1.

4. Paragraph 6.7.3.2.9 defines the strength requirements for portable tanks as whole, with fastenings, and taking into account application of static forces during transportation, which are calculated basing on Maximum Permissible Gross Mass (MPGM).

5. In accordance with 6.7.3.2.9, the head pressure to be used for design pressure is calculated basing on the MPGM instead of a payload directly applied to the walls of the vessel (P impact). To our mind, this follows to the increase of shell thickness and consequently to increase of mass of vessel.

6. It is suggested to calculate the head pressure on the basis of the maximum payload but not on maximum gross mass as stated in 6.7.3.2.9.

 Proposal

7. Bearing in mind the above, it is suggested to amend 6.7.3.1 (ii) as follows:

*“(ii) a head pressure determined on the basis of the static forces ~~specified in 6.7.3.2.9~~ at the direction of travel: (2R-T)g (where R= MPGM, T=tare, g=* *acceleration of gravity), but not less than 0.35 bar.”.*