**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods**

Bern, 12-16 March 2018 **21 December 2017**

Item 4 of the provisional agenda

**Interpretation of RID/ADR/ADN**

 Application of special provision CW24/CV24 – ECE/TRANS/WP.15/AC.1/2018/5

 Transmitted by the Government of Poland

Annex

**2**

|

|  |
| --- |
| UN No. |

 |

|  |
| --- |
| Name and description |

 | Class | Classi-fication code | Packing group | Labels | Special provi-sions | Limited and excepted quantities | Packaging | Portable tanks and bulkk containers | RID/ADR tanks | Trans-port cate-gory/tunnel restri-ctions | Special provisions for carriage | Colis express (express parcels)/SP for carriage/ Operations | Hazard identifica-tion No. |
| Packaging instrucions | Special packing provisions | Mixed packing provisions | Instru-ctions | Special provi-sions | Tank code | Special provisions | Packa-ges | Bulk | Loading, unloading and handling |
|  | 3.1.2 | 2.2 | 2.2 | 2.1.1.3 | 5.2.2 | 3.3 | 3.4/3.5.1.2 | 4.1.4 | 4.1.4 | 4.1.10 | 4.2.5.2,7.3.2 | 4.2.5.3 | 4.3 | 4.3.5,6.8.4 | 1.1.3.1 c)/1.1.3.6 (6.6) | 7.2.4 | 7.3.3 | 7.5.11/8.5 | 7.6 | 5.3.2.3 |
| (1) | (2) | (3а) | (3b) | (4) | (5) | (6) | (7a) | (7b) | (8) | (9а) | (9b) | (10) | (11) | (12) | (13) | (15) | (16) | (17) | (18) | (19) | (20) |
| 1796 | NITRATING ACID MIXTURE with more than 50% nitric acid | 8 | CO1 | I | 8 5.1 |   | 0 | E0 | P001 |   | MP8 MP17 | T10 | TP2 | L10BH | TU38 TC6 TE22 TT1 | 1(E) |   |   | RID: CW24/ADR: CV24 |   | 885 |
| 1796 | NITRATING ACID MIXTURE with not more than 50% nitric acid | 8 | C1 | II | 8 |   | 1 L | E0 | P001 IBC02 |   | MP15 | T8 | TP2 | L4BN |   | 2 |   |   | RID: CW24ADR: - | CE6 | 80 |
| 1826 | NITRATING ACID MIXTURE, SPENT, with more than 50% nitric acid | 8 | CO1 | I | 8 5.1 | 113 | 0 | E0 | P001 |   | MP8 MP17 | T10 | TP2 | L10BH | TU38 TE22 | 1(E) |   |   | RID: CW24/ADR: CV24 |   | 885 |
| 1826 | NITRATING ACID MIXTURE, SPENT, with not more than 50% nitric acid | 8 | C1 | II | 8 | 113 | 1 L | E0 | P001 IBC02 |   | MP15 | T8 | TP2 | L4BN |   | 2(E) |   |   | RID: CW24ADR: - | CE6 | 80 |
| 2031 | NITRIC ACID, other than red fuming, with more than 70% nitric acid | 8 | CO1 | I | 8 5.1 |   | 0 | E0 | P001 | PP81 | MP8 MP17 | T10 | TP2 | L10BH | TU38 TC6 TE22 TT1 | 1(E) |   |   | RID: CW24/ADR: CV24 |   | 885 |
| 2031 | NITRIC ACID, other than red fuming, with at least 65%, but not more than 70% nitric acid | 8 | CO1 | II | 8 5.1 |   | 1 L | E2 | P001 IBC02 | PP81 B15 | MP15 | T8 | TP2 | L4BN |   | 2(E) |   |   |   | CE6 | 85 |
| 2031 | NITRIC ACID, other than red fuming, with less than 65% nitric acid | 8 | C1 | II | 8 |   | 1 L | E2 | P001 IBC02 | PP81 B15 | MP15 | T8 | TP2 | L4BN |   | 2(E) |   |   |   | CE6 | 80 |

\_\_\_\_\_\_\_\_\_\_