|  |  |  |
| --- | --- | --- |
|  | United Nations | ECE/TRANS/WP.15/AC.1/2018/15 |
| _unlogo | **Economic and Social Council** | Distr.: General12 June 2018Original: English  |

**Economic Commission for Europe**

Inland Transport Committee

**Working Party on the Transport of Dangerous Goods**

**Joint Meeting of the RID Committee of Experts and the**

**Working Party on the Transport of Dangerous Goods**

Geneva, 17–21 September 2018

Item 5 (b) of the provisional agenda

**Proposals for amendments to RID/ADR/ADN:**

**new proposals**

 RID/ADR 7.5.2.1 – mixed loading prohibitions for packages for which no danger labels are prescribed

 Transmitted by the Government of Germany [[1]](#footnote-2), [[2]](#footnote-3)\*\*

 Introduction

1. In Germany, the question has arisen in connection with the mixed loading prohibitions of RID/ADR 7.5.2 as to how to deal with packages that contain dangerous goods for which no danger labels are prescribed in Table A of Chapter 3.2 (UN 2211 and UN 3314).

2. Germany is of the view that there are no safety concerns with regard to the mixed loading of UN 2211 and UN 3314 with goods of classes 2 to 9. However, mixed loading with substances and articles of Class 1 should be prohibited, because when UN 2211 and UN 3314 are being carried, there is a risk of an explosive atmosphere developing. In addition, according to the table in RID/ADR 7.5.2.1, mixed loading with substances and articles of Class 1 is only possible to a very limited extent.

 Proposal

3. Insert the following as a second sentence in RID/ADR 7.5.2.1:

“For packages containing dangerous goods for which no danger label is prescribed in Table A of Chapter 3.2, mixed loading with substances and articles of Class 1 shall be prohibited.”

4. Consequential amendment to RID 7.5.2.1:

The current second sentence becomes the third sentence.

 Justification

5. There is no clear statement in RID/ADR 7.5.2.1 concerning mixed loading for packages containing dangerous goods for which no danger label is prescribed in Table A of Chapter 3.2. For safety reasons, there should be such a mixed loading prohibition for substance and articles of Class 1. At present, this only concerns UN Nos. 2211 and 3314 in Table A.

1. In accordance with the programme of work of the Inland Transport Committee for 2018-2019, (ECE/TRANS/2018/21/Add.1, Cluster 9, (9.2)). [↑](#footnote-ref-2)
2. \*\* Circulated by the Intergovernmental Organisation for International Carriage by Rail (OTIF) under the symbol OTIF/RID/RC/2018/15. [↑](#footnote-ref-3)