Submitted by the expert from Germany Informal document **GRSP-65-18rev.1**

(65rd GRSP, 14‐18 May 2018

agenda item 9)

# Proposal for Supplement 5 to the 08 series of amendment to UN Regulation No. 17 and for Supplement 2 to the 09 series of amendment to UN Regulation No. 17 – SEATS, THEIR ANCHORAGES AND ANY HEAD RESTRAINTS

‘

The text reproduced below has been prepared by the expert from Germany to amend the definition of integrated, detachable and separate head restraint. The modifications to the current text of the Regulation are marked in bold for new or strikethrough for deleted characters.

# Proposal

*Paragraph 2.12.1. and 2.12.2., amend to read:*

" 2.12. “Head restraint” means a device whose purpose is to limit the rearward displacement of an adult occupant's head in relation to his torso in order to reduce the danger of injury to the cervical vertebrae in the event of an accident;

2.12.1. "Integrated head restraint" means a head restraint formed by the upper part of the seat-back. ~~Head restraints meeting the definitions of paragraphs 2.12.2. or 2.12.3. below but which can only be detached from the seat or the vehicle structure by the use of tools or by partial or complete removal of the seat covering, meet the present definition;~~

2.12.2. "*Detachable head restraint*" means a head restraint consisting of a component separable from the seat designed for insertion and positive retention in the seat-back structure. **A detachable head restraint, which can only be detached from the seat by the use of tools and/or after partial or complete removal of the seat covering, meet the present definition;"**

*Insert a new paragraph 5.5.6.*

**5.5.5. In the case of a seat with an integrated head restraint, as defined in paragraph 2.12.1. above, the part of the seat-back in a height equal to or greater than 700 mm above the R point at any point between two vertical longitudinal planes passing at 85 mm** **to each side of the vertical median plane of the seat for which the head restraint is intended, shall be viewed as constituting the head restraint.**

1. **Justification**

Clarification with regard to the definition of integrated and detachable head restraints.

The current definition of head restraint was done based on the knowledge of the eighties. The link between integrated and detachable / separate head restraints by the wording "the use of tools or by partial or …" is no longer useful.

Today, the head restraints are an important part of the restraint system of a vehicle and contribute to minimizing the risk of injury in the event of an accident. To meet the current legal requirements for vehicle crashes, stable connections between the components of the restraint systems are required. In that cases the vehicle user shall not be able to detach such detachable or separate head restraints without much effort.

In order

* to avoid the misinterpretation that these stable connections which represents in case of the detachable or separate head restraints a positive retention as defined in 2.12.2 and 2.12.3, leads to an integrated head restraint,
* to describe the definitions clear and distinct,
* to allow future innovative head restraint concepts and
* to be able to prevent vehicle users from taking out head restraints without much effort

the current text of paragraph 2.12.1. and paragraph 2.12.2., should be changed as described above.

Paragraph 2.12.3. "Separate head restraint" means a head restraint consisting of a component separate from the seat, designed for insertion and/or positive retention in the structure of the vehicle; should remain as it is.

In addition the proposal defines in line with UN Global Technical Regulation No. 7, which part of the seat back in case of an integrated head restraint shall be viewed as constituting the head restraint.