|  |  |  |
| --- | --- | --- |
|  | United Nations | ST/SG/AC.10/C.3/2019/15 |
| _unlogo | **Secretariat** | Distr.: General3 April 2019Original: English |

**Committee of Experts on the Transport of Dangerous Goods
and on the Globally Harmonized System of Classification
and Labelling of Chemicals**

|  |
| --- |
| **Sub-Committee of Experts on the Transport of Dangerous Goods**  |
| **Fifty-fifth session** |
| Geneva, 1-5 July 2019Item 3 of the provisional agenda**Listing, classification and packaging** |

 Organic peroxides, new formulations to be listed in 2.5.3.2.4 and portable tank instruction T23

 Transmitted by the European Chemical Industry Council (CEFIC)[[1]](#footnote-2)

 Introduction

1. Since new organic peroxide formulations have become commercially available, there is a need to update the list under 2.5.3.2.4 and portable tank instruction T23. A list of new products, proposed classification, the accompanying competent authority approval references and a summary of the supporting test data are given in the Annex to this document.

 Proposals

1. CEFIC proposes to include a new entry in the list of currently assigned organic peroxide under 2.5.3.2.4 and a new entry to portable tank instruction T23 in 4.2.5.2.6 as follows:

 Amendments to 2.5.3.2.4, list of currently assigned organic peroxides

Add the following new entry for “ACETYL ACETONE PEROXIDE”:

| ORGANIC PEROXIDE | **Concentration (%)** | **Diluent type A (%)** | Diluent type B1  (%) | **Inert solid (%)** | **Water** **(%)** | **Packing Method** | **Control tempe-rature (°C)** | **Emergency temperature  (°C)** | **Number (Generic entry)** | **Subsidiary hazards and remarks** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| " | ≤35 | ≥ 57 |  |  | ≥ 8 | OP8 |  |  | 3107 | 32) |

In the list of “notes on 2.5.3.2.4” add the following entry:

*“32) Active oxygen ≤ 4.15%”*

 Amendments to 4.2.5.2.6, portable tank instruction T23

For UN No. 3109 “ORGANIC PEROXIDE, TYPE F, LIQUID” add “tert-Butyl hydroperoxide, not more than 56% with diluent type Bd” under the column “substance”.

Add a new note “d” under the table to read: “d being tert-Butyl alcohol".

Annex

**ST/SG/AC.10/C.3/2019/15**

 Test results of new organic peroxides and formulations to be added in 2.5.3.2.4 and T23

| **No** | **Product** | **packaging** | **UN** | ***Detonation*** | ***P/T/C.1*** | ***Deflagration/C.2*** | ***Koenen/E.1*** | ***DPVT/E.2*** | ***(mod) Trauzl F.3 or F.4 or F5*** | ***SADT(H.3 or H.4)*** | **Competent authority approval number** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1 | Acetyl Acetone Peroxide | OP8 | 3107 | Test A.1Fragmented length 11 and 13 cmNo | <2170kPa, No | 0.012 mm/s, No | < 1mm(“O”),No | 1.0 mm (10g),Low | F.310 and 15 mlLow | H.460 °C (400ml) | NL TNONL 06DV3/3307 |
| 2 | tert-Butyl hydroperoxide, not more than 56% in a diluent type B | T23portable tank | 3109 | Test A.6Fragmented lenth 19 cm;Blanc 16.5 cmNo  | Max. pressure of 2070 kPa not achieved No | <0.01 mm/s50 °CNo | <1.0mm ("A")Low | 1.0 mm(10g) Low | F.413.8 mlBlanc11.5 ml No | H.3isothermalcalorimetry50°Cfor a 20-m3insulated tank | NL TNO 18EM/0567Test report including emergency vent testing for tank. according to the vent test in Appendix 5 of the Manual of Tests and Criteria, 10 liter vent test for vent sizing |

1. In accordance with the programme of work of the Sub-Committee for 2019-2020 approved by the Committee at its ninth session (see ST/SG/AC.10/C.3/108, paragraph 141 and ST/SG/AC.10/46, paragraph 14) [↑](#footnote-ref-2)