Proposal to amend the text of UN Regulation No. 65 (Special warning lamps)

The text reproduced below was prepared by expert from Poland. The modifications are marked in **bold**.

 I. Proposal

*Paragraph 1.4.* amend to read:

“1.4. The *"on" time* tH means the period of time within which the luminous intensity of the flashing light is superior to 1/10 of the maximum value (peak value) Jm,

**In the case of groups of flashes the "on" time shall be evaluated from the beginning of the first flash of the group to the end of the last flash of the group measured at 1/10 of the maximum value (peak value) Jm.**

 II. Justification

1. The current definition, unlike the one in p. 1.5, is not adapted to the case where a single flash consists of several flashes. It can be interpreted, that it should be a sum of only the “on” time of each flash in group (omitting the gaps between flasches). The amendment aims to clarify the definition due to interpretation problems.