Proposal for amendments to GRE/2019/29

I. Proposal

*Paragraph 5.11. and related sub paragraphs,* amend to read:

# "5.11. The electrical connections shall be such that the front and rear position lamps, the end-outline marker lamps, if they exist, the side-marker lamps, if they exist, and the rear registration plate lamp can only be switched ON and OFF simultaneously.

5.11.1. This ~~condition~~ **requirement** does not apply **while one or more of the following conditions exist**:

~~5.11.1.1.~~ **(a)** ~~When~~ front and rear position lamps ~~are switched ON~~, as well as side-marker lamps when combined or reciprocally incorporated with said lamps, **are switched ON** as parking lamps; ~~or~~

~~5.11.1.2.~~ **(b)** ~~When~~ side-marker lamps flash in conjunction with direction indicators; ~~or~~

 **(c) daytime running lamps are switched ON;**

~~5.11.1.3.~~~~When light signaling system operates according to paragraph 6.19.7.4.~~

Remark:

Correction is necessary because of the agreed change in UN R48.06 based on the proposal GRE/2019/05 from CZ-IT during the 81st session of GRE. The sub-paragraph (c) is equivalent but in different wording.

~~5.11.2.~~ **(d)** ~~to~~ front position lamps ~~when their~~ function is substituted under the provisions of paragraph 5.12.1. below.

5.11.~~3~~**2**. In the case of an interdependent lamp system, all light sources shall be switched ON and OFF simultaneously."

*Paragraph 6.26.7.,* amend to read:

# "6.26.7. Electrical Connections

 Manoeuvring lamps shall be so connected that they cannot be ~~activated~~ **switched ON** unless the main-beam headlamps or the dipped-beam headlamps are switched ON at the same time.

 The manoeuvring lamp(s) shall be ~~activated~~ **switched ON** automatically for slow manoeuvres up to ~~10 km/h~~ 15 km/h provided that one of the following conditions is fulfilled:

Remark:

Correction is necessary because of the agreed change in the complete text from 10 km/h to 15 km/h.

(a) Prior to the vehicle being set in motion for the first time after each manual activation of the propulsion system; or

(b) Reverse gear is engaged; or

(c) A camera based system which assists parking manoeuvres is ~~activated~~ **operating.**

 The manoeuvring lamps shall be automatically switched ~~off~~ **OFF** if the forward speed of the vehicle exceeds ~~10 km/h~~ **15 km/h** and they shall remain switched ~~off~~ **OFF** until the **switch ON** conditions ~~for activation~~ are met again."