**Proposal for Supplement [x] to UN Regulation No. 148 (Light-Signalling Devices)**

I. Proposal:

*Paragraph 3.3.4.5.,* amend to read:

“3.3.4.5. In the case of lamps with light source module(s) on the light source module(s) bear marking of:

(a) The trade name or mark of the applicant;

(b) The specific identification code of the module; This specific identification code shall comprise the starting letters “MD” for “MODULE” followed by the approval mark without the circle as prescribed in paragraph 3.3.2. or by the UI without the truncated circle as prescribed in paragraph 3.3.3.**.**

**In case several non-identical light source modules are used, followed by additional symbols or characters;**

The approval mark or the UI does not have to be the same as the one on the lamp in which the module is used, but both marks shall be from the same applicant;

(c) The rated voltage or the range of voltage.”

II. Justification:

1. In case a signalling device contains more than one different light source modules, which is already foreseen by the Regulation, there was some text missing to differentiate these modules from each other.
2. This proposal adds this missing provision for multiple light source modules that was already present in paragraph 3.6.2. of UN Regulation No. 7.