|  |  |  |  |
| --- | --- | --- | --- |
|  | United Nations | ECE/ADN/54/Add.1 | |
| Description: _unlogo | **Economic and Social Council** | | Distr.: General  29 July 2020  English  Original: English and French |

**Economic Commission for Europe**

**Administrative Committee of the European Agreement   
Concerning the International Carriage of Dangerous  
Goods by Inland Waterways (ADN)**

European Agreement concerning the International Carriage of Dangerous Goods by Inland Waterways (ADN)

Draft amendments to the Regulations annexed to ADN[[1]](#footnote-2)\*

Addendum

Chapter 1.1

1.1.3.7 (b) At the end, add “, except for equipment such as data loggers and cargo tracking devices attached to or placed in packages, overpacks, containers or load compartments which are only subject to the requirements in 5.5.4”.

Chapter 1.2

1.2.1 Amendment to the definition of *Membrane tank* does not apply to the English text.

Chapter 1.4

1.4.3.3 (b) Replace “test” by “inspection”.

1.4.3.4 (a) Replace “tests” by “inspections, tests”.

1.4.3.4 (b) The amendment does not apply to the English text.

Chapter 1.10

Table 1.10.3.1.2

For Class 6.2, in column “Substance or article”, at the end, add “and medical waste of Category A (UN No. 3549)”.

Chapter 2.2

2.2.41.1.10 The amendment does not apply to the English text.

2.2.62.1.11.1 Amend to read as follows:

“2.2.62.1.11.1 Medical or clinical waste containing:

(a) Category A infectious substances shall be assigned to UN No. 2814, UN No. 2900 or UN No. 3549, as appropriate. Solid medical waste containing Category A infectious substances generated from the medical treatment of humans or veterinary treatment of animals may be assigned to UN No. 3549. The UN No. 3549 entry shall not be used for waste from bio-research or liquid waste;

(b) Category B infectious substances shall be assigned to UN No. 3291.

***NOTE 1***: *The proper shipping name for UN No. 3549 is "MEDICAL WASTE, CATEGORY A, AFFECTING HUMANS, solid" or "MEDICAL WASTE, CATEGORY A, AFFECTING ANIMALS only, solid".*”.

Renumber existing Note as Note 2.

Chapter 3.2, Table A

Add the following new entries in proper order:

| (1) | (2) | (3a) | (3b) | (4) | (5) | (6) | (7a) | (7b) | (8) | (9) | (10) | (11)  HA01, HA02, HA03  HA01, HA02, HA03  HA01, HA03 | | | (12) | (13) |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 0511 | DETONATORS, ELECTRONIC programmable for blasting | 1 | 1.1B |  | 1 |  | 0 | E0 |  | PP |  | LO01 | HA01, HA02, HA03 |  | 3 |  |
| 0512 | DETONATORS, ELECTRONIC programmable for blasting | 1 | 1.4B |  | 1.4 |  | 0 | E0 |  | PP |  | LO01 | HA01, HA02, HA03 |  | 1 |  |
| 0513 | DETONATORS, ELECTRONIC programmable for blasting | 1 | 1.4S |  | 1.4 | 347 | 0 | E0 |  | PP |  | LO01 | HA01, HA03 |  | 0 |  |
| 3549 | MEDICAL WASTE, CATEGORY A, AFFECTING HUMANS, solid or MEDICAL WASTE, CATEGORY A, AFFECTING ANIMALS only, solid | 6.2 | I3 |  | 6.2 | 395 802 | 0 | E0 |  | PP |  |  |  |  | 0 |  |

Chapter 3.3

SP 658 Replace “EN ISO 9994:2006 + A1:2008” by “EN ISO 9994:2019”.

SP 672 At the beginning, replace “Machinery and apparatus” by “Articles, such as machinery, apparatus or devices”. In the second indent, replace “machinery or apparatus” by “article”.

Chapter 5.4

5.4.1.2.2 (d) Replace “tank-containers” by “tank-wagons, tank-containers or portable tanks”.

Chapter 5.5

5.5.4 Add a new section 5.5.4 to read as follows:

“**5.5.4 Dangerous goods contained in equipment in use or intended for use during carriage, attached to or placed in packages, overpacks, containers or load compartments**

5.5.4.1 Dangerous goods (e.g. lithium batteries, fuel cell cartridges) contained in equipment such as data loggers and cargo tracking devices, attached to or placed in packages, overpacks, containers or load compartments are not subject to any provisions of ADN other than the following:

(a) the equipment shall be in use or intended for use during carriage;

(b) the contained dangerous goods (e.g. lithium batteries, fuel cell cartridges) shall meet the applicable construction and test requirements specified in ADN; and

(c) the equipment shall be capable of withstanding the shocks and loadings normally encountered during carriage and shall be safe for use in the dangerous environments to which it may be exposed.

5.5.4.2 When such equipment containing dangerous goods is carried as a consignment, the relevant entry of Table A of Chapter 3.2 shall be used and all applicable provisions of ADN shall apply.”.

1. \* Distributed in German by the Central Commission for the Navigation of the Rhine under the symbol CCNR/ZKR/ADN/54/Add.1. [↑](#footnote-ref-2)